Weitek P9100-Based Display Adapter
¬

¬ Display Devices

This device driver is for VL-Bus systems.  

Supported Hardware: 
	Weitek P9100 based display adapters with 2MB memory

This graphics driver is designed to support VL-bus and PCI-bus display controller subsystems based on the P9100 graphics controller from Weitek.

This driver supports the following 2MB display modes. 
	
8-bit Color	16-bit Color	32-bit color
	
		640-x480
		60 Hz

800x600 	800x600  	800x600
60, 72, 75 Hz	60, 72, 75 Hz	60, 72, 75 Hz
	
1024x768 	1024x768
60, 70, 75 Hz	60, 70, 75 Hz
	
1152x896	1152x896
60, 70, 75 Hz	60, 70, 75 Hz

1280x1024
60, 72, 75 Hz

1600x1200
60 Hz

Supported Displays:  NeXT designs and tests its display adapter device drivers using very high frequency displays that can support display modes with very high resolutions and non-interlaced refresh rates, such as the NEC 5FG, NEC 6FG, and Nokia Multigraph 445X.  Read the owner's guide that comes with your display to ensure it can support the display mode you set in Configure.

Warning:  Some vendors claim that you can use their display adapters at display modes with resolutions and refresh rates that exceed what their RAMDACs can support.  You can permanently damage your display adapter and computer by doing this.  Read the owner's guide that comes with your display adapter or contact its manufacturer to ensure that your adapter's RAMDAC can support the display mode you set in Configure.

Warning:  If you plan to change display adapters, be sure to use the Configure application to change the display driver to Default VGA Adapter before you remove the old display adapter (see NeXTanswer 1824 for details on changing display adapters). 

¬

See also

·	"Add a Device" in Configure's on-line help.

·	See NeXTanswer 1824 for general information on installing and configuring device drivers.