Beep When Drops Occur

To make it easier to notice that a drop occurred on a busy bus, choose Beep when drops occur.  MacPing will give a short beep the first time a device fails to reply to a probe packet.