DEFINITION MODULE Keyboard;

        (************************************************)
        (*                                              *)
        (*      Module to deal with keyboard input.     *)
        (*                                              *)
        (*  Programmer:         P. Moylan               *)
        (*  Last edited:        19 December 1997        *)
        (*  Status:             OK                      *)
        (*                                              *)
        (************************************************)

FROM Semaphores IMPORT
    (* type *)  Semaphore;

PROCEDURE KeyPressed(): BOOLEAN;

    (* Returns TRUE iff a character is available. *)

PROCEDURE InKey (): CHAR;

    (* Reads a single character code from the keyboard. *)

PROCEDURE PutBack (ch: CHAR);

    (* This is an "un-read" operation, i.e. the character ch will       *)
    (* re-appear on the next call to InKey.  This facility is provided  *)
    (* for the use of software which can overshoot by one character     *)
    (* when reading its input - a situation which can often occur.      *)
    (* Some versions of this module will allow several calls to PutBack *)
    (* before the next call to InKey, but no guarantee is made in that  *)
    (* case of uniform treatment from version to version.               *)

PROCEDURE StuffKeyboardBuffer (ch: CHAR);

    (* Stores ch as if it had come from the keyboard, so that a         *)
    (* subsequent InKey() will pick it up.                              *)

    (* NOTE: Procedures PutBack and StuffKeyboardBuffer do almost the   *)
    (* same thing, but not quite.  The differences are:                 *)
    (*  1. StuffKeyboardBuffer stores characters in a first-in-first-out*)
    (*     order, whereas PutBack uses last-in-first-out.               *)
    (*  2. StuffKeyboardBuffer is intended for the case of a task       *)
    (*     sending data to another task (where that other task is       *)
    (*     expecting keyboard input), and PutBack is designed for the   *)
    (*     case of a task talking to itself (i.e. the PutBack(ch) and   *)
    (*     the InKey() are in the same task).  If you get this the      *)
    (*     wrong way around then you could have timing-related          *)
    (*     problems, up to and including deadlock.                      *)

PROCEDURE StuffKeyboardBuffer2 (ch: CHAR);

    (* Like StuffKeyboardBuffer, but stores a two-byte sequence: Nul    *)
    (* followed by ch.                                                  *)

PROCEDURE SetLocks (code: CARDINAL);

    (* Set/clear the caps lock, num lock, and scroll lock conditions.   *)
    (* The code is defined in KBDRIVER.DEF.                             *)

PROCEDURE LockStatus (): CARDINAL;

    (* Returns the current state of the caps lock, num lock, and scroll *)
    (* lock conditions, using the code defined in KBDRIVER.DEF.         *)

PROCEDURE HotKey (FunctionKey: BOOLEAN;  code: CHAR;  S: Semaphore);

    (* After this procedure is called, typing the key combination for   *)
    (* 'code' will cause a Signal(S).  Set FunctionKey=TRUE to trap one *)
    (* of the two-character special function keys, and FALSE otherwise. *)
    (* The character is consumed; if it should be passed on, then the   *)
    (* user's hot key handler can do a PutBack().  Note: there is no    *)
    (* provision for having multiple hot key handlers for the same key; *)
    (* any existing hot key mapping will be overridden.                 *)

PROCEDURE NotDetached(): BOOLEAN;

    (* Returns TRUE unless called by a process running detached.        *)
    (* (A detached process may not do keyboard, screen, or mouse I/O.)  *)

END Keyboard.

