SOFTWARE PREINSTALLED ON 500-17N (after July 1, 1994) and 510Cs

IBM DOS 6.3, Windows 3.1, Demo, and 8 appls: Lotus cc:Mail, Lotus Organizer 1.12, Lotus ScreenCam 1.0, Official Airline Guide Flight Disk 1.0, Triton CoSession Host, PRODIGY, America Online, SofNet FaxWorks 3.0

EasyPlaying (PC Card Director™ ) is preloaded and on the utility diskette for DOS, Windows and OS/2; it provides status and info on PCMCIA cards installed. In Windows and OS/2, it can register an appl for PCMCIA cards and execute them automatically. Auto Configurator and Memory Device Driver enables supported PCMCIA cards by sensing them automatically (so do not need to install their device drivers).

All: 80486 SL (no math co) All: 25 MHz All: 8 KB internal (no L2) All: No All: 3.5" 1.44 MB

$ 1,499 $ 1,899 2618-J0A 2618-L0A 125 MB 250 MB 15 ms 12 ms June 93 / withd Sep 94

VGA mono 64 grey scales STN LCD - Backlit 9.5 inch 18 to 1 Yes (external SVGA)

All: 65530 / External VGA is ISO capable (75Hz) All: Chips & Tecnologies, Inc. All: Local bus / 16 bit / Peripheral Interface

All: 4 / 20 MB 80 ns All: 1 socket (non-parity) All: 4, 8, 16 MB SIMMs

All: Full size alp/num/ 85 All: 2 (in any appl) All: Yes (back panel) All: TrackPoint II™ All: Yes (with opt cable)

11.7 x 8.3 x 1.9" 184 inches Many options Black 5.2 pounds

Nickel hydride (NiMH) 2.7 to 9 hours 2 hrs / 1 hr

All: AT bus (ISA) All: No All: No All: Modem only All: 1 Type I or 1 Type II All: Yes All: Yes / Yes

All: APM-aware BIOS All: Wallmount AC adapter

All: Personalized nameplate in indentation All: Coupon book with $4,000 in savings All: IBM DOS 5.02, PRODIGY^®

All: 1 year - carry in or EasyServ(opt onsite)

$ 1,599 $ 1,999 2618-N0A 2618-P0A 125 MB 250 MB 15 ms 12 ms June 93 / withd Sep 94

VGA color 256 colors 640 x 480 STN - passive matrix LCD - Backlit 9.2 inch 13 to 1; Single scan Yes (external SVGA)

11.7 x 8.3 x 2.0" 194 inches Many options Black 5.8 pounds

Nickel hydride (NiMH) 2 to 7.5 hours 2 hrs / 1 hr

Blue Lightning 486BL2-50 50/25 MHz 16 KB internal (no L2 cache) No External 3.5" 1.44 MB (9 oz.)

$ 1,799 2604-C2U 200 MB 17 ms June 94

VGA color 256 colors 640 x 480 STN - passive matrix LCD - backlit 7.7 inch 14 to 1; Single scan Yes (external SVGA)

WD90C24A2 / 1 MB video mem Western Digital VL-Bus / VESA 32 bit local bus

4 / 20 MB 80 ns 1 socket (non-parity) 4, 8, 16 MB ICs (3.3 volt)

90% size alp/num/ 81 15 (in any appl) No TrackPoint II Yes (on MultiPort)

10.1 x 7.2 x 1.7" 124 inches Many options Black 4.0 pounds

Nickel hydride (NiMH) 2.5 to 8 hours 2.5 hrs / 1.5 hrs

AT bus (ISA) No Yes (MultiPort ships standard) No 1 Type I or 1 Type II Yes Yes (MultiPort) / Yes (EPP)

APM-aware BIOS Microsaver™ security connector Hibernation mode Personalized nameplate in indentation Personal greeting screen at startup IBM DOS 6.3, Windows 3.1, Demo, and 8 appls listed below

1 year - carry in or EasyServ(optional onsite for $40 a year)

IBM ThinkPad 350, 350C, 500, 510Cs

IBM^® ThinkPad^® :

Processor type Processor speed Memory cache Coprocessor socket Diskette drive

Price (retail USD) Type - model Hard drive - size Hard drive - speed Avail / withdrawal date

Display - type Display - grey scales Display - techology Display - light source Display - size (diag) Display - contrast ratio 180 degree display tilt

Graphics - controller Graphics - vendor Graphics - arch/data path

Memory - std / max Mem - sockets empty Mem - options available

Keyboard / # of keys Fn key functions Keyboard slope Mouse/pointing Ext keyboard support

Dimensions Cubic inches Carrying case Color Weight (with battery)

Battery - type Batt - life (per battery) Charge time - on / off

Architecture Docking Station Port replicator Modem/serial slot PCMCIA 2.01 slots Visible LEDs - closed Serial / parallel ports

APM-aware BIOS Other features

Preinstalled software

Warranty

80486 SLC2 50/25 MHz 16 KB internal (no L2) No External 3.5" 1.44 MB

$ 799 $ 999 2603-08N 2603-17N 85 MB 170 MB 15 ms 15 ms Dec 93 Dec 93

VGA mono 64 grey scales STN LCD - backlit 7.24 inch 18 to 1 Yes (external SVGA)

WD90C26 Western Digital ISA 16 bit

4 / 12 MB 80 ns 1 socket (non-parity) 4, 8 MB ICs (3.3 volt)

90% size alp/num/ 81 11 (in any appl) No TrackPoint II No 10.1 x 7.2 x 1.6" 116 inches Many options Black 3.4 pounds / 3.7 (170M)

Nickel hydride (NiMH) 3.5 to 9 hours 3 hrs / 1.5 hrs

AT bus (ISA) No No No 1 Type I or 1 Type II Yes Yes (cable) / Yes (EPP)

APM-aware BIOS

Hibernation mode Personalized nameplate Coupon book w/ sav IBM DOS 6.1,PRODIGY After July 1 only on 17N: see below 1 year - carry in or EasyServ(opt onsite)

350 monochrome

Suspend/resume buttn above keyboard Fn+F1=Configuration Utility Fn+F2=Reverse video Fn+F3=Contrast text

500 sub-notebook

510Cs color sub-notebook

ThinkPad EasyServ ™ : customer calls 1-800-772-2227, courier service picks up ThinkPad at any location, IBM repairs and mails back (no shipping charges, most shipping is overnight, 4 business days total ). = Upgradeable; Price decrease effective July 13 (350C) and Aug 18 (510), 1994.

All trademarks are the property of their respective owners No warranties are expressed or implied in this summary (1THINK) Compiled by Roger Dodson, IBM. September 1994

Fn+F2 = Fuelguage Fn+F3 = Setup Fn+F4 = Suspend Fn+F5 = Speaker Fn+F6 = Sysrequest Fn+F7 = CRT/LCD Fn+F8 = Rev video Fn+F9 = Num Lock Fn+F10= Scroll Lock Fn+F11= Print Scrn Fn+F12= Hibernation

350C passive color

Fn+Q=Inc brightness Fn+A=Dec brightness Fn+W=Inc contrast Fn+ S =Dec contrast

Enter Setup by CTRL+ALT+F3 from DOS prompt

(withdrawn 500 had sealed lead acid battery)

FEATURES OF 500 and 510Cs FEATURES OF ALL PRODUCTS

Suspend/resume mode; battery life indicator Non-disruptive battery exchange Simultaneous LCD and external CRT US EPA Energy Star compliant International travelers warranty IBM or dealer warranty/service 30 day money back guarantee 24 hour / 7 day fax support 24 hour / 7 day bulletin board support 24 hour / 7 day telephone support at 1-800-772-2227

ThinkPad 500 memory (4, 8 MB IC 3.3 volt) is compatible with ThinkPad 510Cs.

ThinkPad 510Cs MultiPort is NOT compatible with ThinkPad 500.

500: External cable has 2 connectors for

serial port and external diskette drive 510: External cable has 1 connector for

external diskette drive (serial port on MultiPort).

MultiPort: A port replicator with connectors fordiskette drive, external display, mouse/ keyboard, and serial device (ships with 510Cs). Plugs into 160 pin connector on back.

3 power saving modes: doze, suspend, hibernation.

Batteries in 500 and 510Cs are NOT compatible

Withdrawn from marketing

?