IBM SCSI Disks - withdrawn

All trademarks are the property of their respective owners (listed on Trademark sheet) Price decrease effective June 16, 1994

No warranties are expressed or implied in this summary (3SCSI) Compiled by Roger Dodson, IBM. September 1994

Capacity Interface SCSI data path SCSI burst rate Buffer size Buffer type (no. of segments)

Buffer write caching Average seek time (ms) Average latency Rotational speed Media transfer rate Mean Time Between Failure Form factor (width x height) Tagged Command Queueing Automatic Defect Reallocation Predictive Failure Analysis Head technology Vendor Available date Withdrawal date Part number (old) Part number (new) Price (retail USD) Part number for 95 A or 3516 with carrier unit/housing Price (retail USD)

170 MB SCSI-2 Fast 8 bit 10 MB/sec 64 KB Read ahead (1)

No (read only) 13 ms 7.5 ms 4011 rpm 3.5 MB/sec 250,000 hrs 3.5" x 1" SL No Yes No Metal in gap Conner February 1994 September 1994 N/A 70G8480 $ 279 None N/A

340 MB SCSI-2 Fast 8 bit 10 MB/sec 64 KB Read ahead (1)

No (read only) 13 ms 7.5 ms 4011 rpm 3.5 MB/sec 250,000 hrs 3.5" x 1" SL No Yes No Metal in gap Conner February 1994 September 1994 N/A 70G8481 $ 455 None N/A

540 MB SCSI-2 Fast 8 bit 10 MB/sec 256 KB Segmented (4)

No (read only) 8.7 ms 4.76 ms 6300 rpm 3.8 MB/sec 300,000 hrs 3.5" x 1" SL Yes Yes No Metal in gap Maxtor July 1993 September 1994 32G4151 70G8491 $ 519 70G7163

$ 609