80486SX (3.3 volt SL Enhanced) 33 MHz 8 KB internal (no L2 cache) No Optional 3.5" 1.44 MB (same as ThinkPad 710T) $ 2,569 $ 2,879 $ 3,119 $ 3,429 2524-801 2524-901 2524-80F 2524-90F Option (required Option (required 105 MB PCMCIA 105 MB PCMCIA via PCMCIA disk) via PCMCIA disk) 15 ms 15 ms IBM DOS 6.3 IBM DOS 6.3 Windows for Pen Computing Windows for Pen Computing May 1994 May 1994 May 1994 May 1994 4 / 20 MB 8 / 24 MB 4 / 20 MB 8 / 24 MB Uses a specific Type III PCMCIA slot; this will then permit a Type I or II PCMCIA card in rest of slot 70 ns / Non-parity / 5.0 volt 4, 8, 16 MB ICs (same options as ThinkPad 360) VGA 640 x 480 monochrome 16 grey scales STN Transflective LCD - Backlit 9.5 inch 3 to 1 External (any IBM keyboard is supported; attach to port replicator) Electromagnetic pen/digitizer/stylus that realistically simulates the feel of pen-to-paper / untethered / batteryless (a mouse is not supported) / stylus is stored in a compartment on bottom 10.6 x 8.3 x 1.4" 123 inches Blk nylon standard (many options also available) Black 3.5 pounds (1 battery); 3.9 pounds (2 batteries) Nickel hydride Two batteries ship standard / can use one or two batteries 1 battery: 2 to 5 hours 2 battery: 4 to 10 hours N/A / 1.5 hours (unit off or suspend only) Local memory bus / ISA No Yes (ships standard / attach to 200 pin connector) Port Replicator includes 15 pin external CRT port, 9 pin 16550A serial port, 25 pin EPP parallel port, diskette drive connector, keyboard port, DC port for AC connector No (use PCMCIA) 3 Type II or 2 Type III as follows:

1st slot: 2 Type II or 1 Type III (but any additional memory must go into this slot; so adding IC DRAM memory will leave 1 Type II slot remaining) 2nd slot: 2 Type II or 1 Type III (105 MB PCMCIA disk in Models 80F/90F is installed here) Yes (on Port Replicator) / Yes (on Port Replicator) 3 year - ThinkPad EasyServ™ only: customer calls 1-800-772-2227, courier service picks up ThinkPad at any location, IBM repairs and mails back within 4 business days (no shipping charges, most shipping is overnight) Includes International Travelers Warranty

Options: Description

Quick Charger Car Adapter NiMH Battery (dual) AC Adapter PortReplicator External 3.5" 1.44 MB diskette drive 105 MB HDD (PenDOS) 105 MB HDD (PenOS2) Hand Strap Soft Case Battery Carrier

Part number

66G9540 66G9545 66G9550 84G0480 84G0485 48G8263 84G9180 84G9190 84G0495 84G0490 84G0500

Cost 155 175 189 135 139 275 549 549 25 99 19

IBM ThinkPad 730T

Processor type Processor speed Memory cache Coprocessor socket Diskette drive Price (retail USD) Type - model Hard drive - size Hard drive - speed Preinstalled software

Available date Memory - std / max Mem - sockets empty Memory - type Memory - options Display - type Display - grey scales Display - techology Display - light source Display - size (diag) Display - contrast ratio Keyboard Mouse/pointing

Dimensions Cubic inches Carrying case Color Weight (with battery) Battery - type Battery - quantity Batt - life (per battery)

Charge time - on / off Architecture Docking Station Port replicator

Modem/serial slot PCMCIA 2.01 slots

Serial / parallel ports Warranty

IBM^® ThinkPad^® : 730T pen tablet

The ThinkPad 730T requires a bootable operating system with Pen capability. Supported is:

� PenDOS^® 2.2 with IBM DOS 6.3

84G9180 - PCMCIA HDD 105 MB PenDOS preloaded � Pen for OS/2 1.0 with OS/2^® 2.11

84G9190 - PCMCIA HDD 105 MB Pen for OS/2 preloaded � Windows for Pen Computing^® 3.1 with IBM DOS 6.3

Models 80F/90F are preloaded with Windows for Pen Computing � PenRight! ^® (available at dealers)

(External display is 640 x 480 with 16 colors) (Simultaneous LCD and CRT display)

Transflective: can turn on backlight in dark areas or turn it off in bright areas

No warranties are expressed or implied in this summary (730THINK) Compiled by Roger Dodson, IBM. May 1994

All trademarks are the property of their respective owners

$ FEATURES OF THINKPAD 730T Suspend/resume mode Battery life indicator Non-disruptive battery exchange US EPA Energy Star compliant IBM or dealer warranty/service 30 day money back guarantee 24 hour / 7 day fax support 24 hour / 7 day bulletin board support 24 hour / 7 day telephone support at 1-800-772-2227

PCMCIA SLOT CONFIGURATION

PCMCIA Type III 105 MB disk in this slot (Models 80F and 90F)

Two Type III (10 mm high):

IC DRAM only