8.4” color active matrix LCD - 8 bit (256 color) Display.

The built-in video is non-upgradeable and supports only 8-bit (256 colors) video on a number of monitors.

A Display adapter is required to use Multiple Scan Monitors at 832 x 624 resolution.