%% This document created by Scientific Notebook (R) Version 3.0


\documentclass[12pt,thmsa]{article}
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\usepackage{sw20jart}

%TCIDATA{TCIstyle=article/art4.lat,jart,sw20jart}

%TCIDATA{<META NAME="ViewSettings" CONTENT="31">}
%TCIDATA{<META NAME="GraphicsSave" CONTENT="32">}
%TCIDATA{<META NAME="Title" CONTENT="Units of Measure">}
%TCIDATA{Created=Mon Aug 19 14:52:24 1996}
%TCIDATA{LastRevised=Mon Mar 31 16:03:19 1997}
%TCIDATA{Language=American English}
%TCIDATA{CSTFile=booklet.cst}
%TCIDATA{PageSetup=61,61,114,114,1}
%TCIDATA{<LINK REL="author" HREF="GSfront.tex">}
%TCIDATA{<LINK REL="first" HREF="GSCompute.tex">}
%TCIDATA{<LINK REL="contents" HREF="GScontents.tex">}
%TCIDATA{<LINK REL="copyright" HREF="GSfront.tex">}
%TCIDATA{<LINK REL="end" HREF="GSCompute15.tex">}
%TCIDATA{<LINK REL="index" HREF="GSindex.tex">}
%TCIDATA{<LINK REL="next" HREF="GSCompute15.tex">}
%TCIDATA{<LINK REL="parent" HREF="GSCompute.tex">}
%TCIDATA{<LINK REL="previous" HREF="GSCompute13.tex">}
%TCIDATA{<LINK REL="publisher" HREF="GSfront.tex">}
%TCIDATA{<LINK REL="top" HREF="GScontents.tex">}
%TCIDATA{<LINK REL="trademark" HREF="GSfront.tex">}
%TCIDATA{AllPages=
%H=78,\PARA{038<p type="texpara" tag="Body Text" >\hfill Getting Started with Scientific Notebook}
%F=36
%}


\input{tcilatex}
\begin{document}


\subsection{Units of Measure\label{Units of Measure}\hrulefill}

In \textit{Scientific Notebook,} you can convert values from one unit of
physical measure to another and you can perform computations on equations
containing units.

\subparagraph{\FRAME{itbpF}{50.75pt}{21.75pt}{6pt}{}{}{ex3.wmf}{\special%
{language "Scientific Word";type "GRAPHIC";display "PICT";valid-file
"F";width 50.75pt;height 21.75pt;depth 6pt;original-width
48.875pt;original-height 19.5625pt;cropleft "0";croptop "1";cropright
"1";cropbottom "0";filename 'ex3.WMF';file-properties "XNPEU";}}Convert $\
28.6\unit{lb}$ to newtons}

\begin{enumerate}
\item  Click\FRAME{itbpF}{20.125pt}{20.125pt}{2pt}{}{}{text.wmf}{\special%
{language "Scientific Word";type "GRAPHIC";maintain-aspect-ratio
TRUE;display "PICT";valid_file "F";width 20.125pt;height 20.125pt;depth
2pt;original-width 16.0625pt;original-height 16.0625pt;cropleft "0";croptop
"1";cropright "1";cropbottom "0";filename 'text.wmf';file-properties
"XNPEU";}}or, from the Insert menu, choose Math to start mathematics.

\item  Type \textbf{28.6}; then click\FRAME{itbpF}{21.75pt}{21.0625pt}{2pt}{%
}{}{units.wmf}{\special{language "Scientific Word";type
"GRAPHIC";maintain-aspect-ratio TRUE;display "PICT";valid_file "F";width
21.75pt;height 21.0625pt;depth 2pt;original-width 19.5625pt;original-height
18.8125pt;cropleft "0";croptop "1.0079";cropright "1.0051";cropbottom
"0";filename 'Units.wmf';file-properties "XNPEU";}}or, from the Insert menu,
choose Unit Name.

\item  Select Force, select Pound, and then choose Insert.

\item  Type \textbf{=x}; then in the Unit Name dialog, select Force, select
Newton, and then choose Insert.

\item  From the Maple menu, choose Solve and then choose Exact. Maple
performs the conversion and returns this result:\medskip\ 
\[
\fbox{%
\begin{tabular}{lll}
\rule[-0.1in]{0in}{0.3in} & $28.6\unit{lb}=x\unit{N}$, Solution is : $%
\left\{ x=127.\,22\right\} $ & \rule[-0.1in]{0in}{0.3in}%
\end{tabular}
}
\]
\end{enumerate}

\subparagraph{\FRAME{itbpF}{50.75pt}{21.75pt}{6pt}{}{}{ex3.wmf}{\special%
{language "Scientific Word";type "GRAPHIC";display "PICT";valid-file
"F";width 50.75pt;height 21.75pt;depth 6pt;original-width
48.875pt;original-height 19.5625pt;cropleft "0";croptop "1";cropright
"1";cropbottom "0";filename 'ex3.WMF';file-properties "XNPEU";}}Express $20.0%
\unit{mi}/\unit{h}$ in kilometers/minute}

\begin{enumerate}
\item  Click\FRAME{itbpF}{20.125pt}{20.125pt}{2pt}{}{}{text.wmf}{\special%
{language "Scientific Word";type "GRAPHIC";maintain-aspect-ratio
TRUE;display "PICT";valid_file "F";width 20.125pt;height 20.125pt;depth
2pt;original-width 16.0625pt;original-height 16.0625pt;cropleft "0";croptop
"1";cropright "1";cropbottom "0";filename 'text.wmf';file-properties
"XNPEU";}}or, from the Insert menu, choose Math to start mathematics.

\item  Type \textbf{20.0}; then click\FRAME{itbpF}{21.75pt}{21.0625pt}{2pt}{%
}{}{units.wmf}{\special{language "Scientific Word";type
"GRAPHIC";maintain-aspect-ratio TRUE;display "PICT";valid_file "F";width
21.75pt;height 21.0625pt;depth 2pt;original-width 19.5625pt;original-height
18.8125pt;cropleft "0";croptop "1.0079";cropright "1.0051";cropbottom
"0";filename 'Units.wmf';file-properties "XNPEU";}}or, from the Insert menu,
choose Unit Name.

\item  Select Length, select Mile, and then choose Insert.

\item  Type \textbf{/}.

\item  In the Unit Name dialog, select Time, select Hour, and then choose
Insert.

\item  Type \textbf{=x}; then in the Unit Name dialog, select Length, select
Kilometer, and then choose Insert.

\item  Type \textbf{/.}

\item  In the Unit Name dialog, \ select Time, select Minute, and then
choose Insert.

\item  From the Maple menu, choose Solve, and then choose Exact. Maple makes
the conversion: \medskip 
\[
\fbox{%
\begin{tabular}{lll}
\rule[-0.1in]{0in}{0.3in} & $20.0\unit{mi}/\unit{h}=x\unit{km}/\unit{mn}$,
Solution is : $\left\{ x=.\,53633\right\} $ & \rule[-0.1in]{0in}{0.3in}%
\end{tabular}
}
\]
\medskip 
\end{enumerate}

\subparagraph{Convert these units of measure\textit{\label{exercises}}}

\begin{quotation}
\qquad Express $53.7\unit{lb}/\unit{in}^{2}\ $in newtons per square
meter\medskip .

\qquad Compute $3\unit{A}6\unit{V}$, then convert the answer to
watts\medskip .

\qquad Convert $3.7\unit{N}/\unit{cm}^{2}$ to pounds per square inch.
\end{quotation}

\end{document}
