Resistivity Logs measure the resistance of the formation rock and to the flow of electrical current.  In many producing areas, oil is much more resistive than the salt water in the formation.  However, Nevada's formation waters are generally very fresh and there is negligible difference in resistivity between the water and oil zones.  The resistivity log is usually run with an SP log which may indicate formation permeability.