The initial production of an oil well recorded after testing operations, which should approximate closely the maximum rate which a well will produce on completion without subsequent reservoir damage.