The liquid that is circulated through the wellbore during drilling operations.  Drilling mud brings cuttings to the surface, cools and lubricates the bit and drill stem, protects against blowouts by holding back subsurface pressures, and deposits a mud cake on the wall of the borehole to prevent loss of fluids to the formations.