A small-diameter pipe that is run inside the casing in a well to serve as a conduit for the passage of oil and gas to the surface.