InS_StArT
TOKEN.COM
1.0
^IBM Token-Ring Network Adapter II & 16/4 Adapter,TOKEN.COM,IE0
^IBM Token-Ring Network Adapter/A,TOKEN.COM,00M,E000
^IBM Token-Ring Network 16/4 Adapter/A,TOKEN.COM,00M,E001
!RIE0(PORT)
@A20
A24
!R00M(SLOT)
1
2
3
4
5
6
7
8
$OIEM(NODE ADDRESS)
0
FFFFFFFFFFFF
$OIEM(MAX FRAME SIZE)Maximum Frame Size
?The maximum frame size must be a multiple of 8.
632
17960
@4208
*RIEM(FRAME)
@TOKEN-RING MSB
TOKEN-RING LSB
TOKEN-RING_SNAP MSB
TOKEN-RING_SNAP LSB
InS_EnD
