Release 3.3 Copyright ã1994 by NeXT Computer, Inc.  All Rights Reserved.

G	Annotated uucico Debug Output

If you are having difficulties with UUCP, you can execute uucico directly to examine detailed debugging information. This appendix contains sample annotated output of the command /usr/lib/uucp/uucico -r1 -x6 -srhino.

This command executes uucico at debug level 6 to the remote site rhino. For more information, see the UNIX manual page for uucico.

root rhino (7/18-09:26-4187) DEBUG (Local Enabled)	Time stamp, noting debugging.
finds (rhino) called	Found system rhino.
getto: call no. cua for sys rhino	No phone number found for rhino.
Using DIR to call	Using a direct connection.
Opening /dev/cufa	Using /dev/cufa.
login called	Beginning login sequence from L.sys.
ABORT ON: BUSY	Abort enabled (abort call if ªBUSYº received).
wanted """"	Wanted nothing.
got: that	Received what was expected.
send "AT"	Sending the AT command.
wanted "OK~3"	Wait 3 seconds for ªOK.º
AT	Modem echoes ªAT.º
OKgot: that	Received ªOKº from modem, as expected.
send "ATX3s50=255"	Send more modem commands.
wanted "OK~3"	Wait 3 seconds for acknowledgment.

>ATX3s50=255	The > is the modem prompt.
OKgot: that
send "ATdt9w1-800-555-1212"	Dial the phone number.
wanted "CONNECT~80"	Wait 80 seconds for ªCONNECT.º

>ATdt9w1-800-555-1212
CONNECTgot: that	Received ªCONNECTº from modem, as 
	expected.
send "PAUSE"	Wait 3 seconds.
wanted "ogin:~15"	Wait 15 seconds for login prompt.
FAST/UUCP/COMP	Part of the modem's connect message.

NeXT Mach (rhino) (ttyda)	Prompt sequence begins. If it hadn't, might have
	sent a newline (CR), or a BREAK.

rhino login:got: that	Got a prompt (ªogin:º).
send "Umyhost"	Log in by sending user name and password.
wanted "ssword:~10"
Umyhost
Password:got: that
send "a5c#.9jq@Z"
root rhino (7/18-09:27-4187) SUCCEEDED (call to rhino)	Completed dialog from L.sys.
imsg looking for SYNC<	Looking for an initial greeting from remote 
\20>	UUCP (all before the normal data transmission
	protocol starts).
imsg input<Shere=rhino\0>got 11 characters	What was received.
omsg <Smyhost -Q0 -x6>	Sending this back, identifying ourselves, at 
	debug level 6.
imsg looking for SYNC<	Looking for an acknowledgment of receipt.
\20>
imsg input<ROK\0>got 3 characters	Got the acknowledgment.
msg-ROK
Rmtname rhino, Role MASTER,  Ifn - 5, Loginuser - root	Initial connection complete.
rmesg - 'P' imsg looking for SYNC<\20>	Begin negotiating data transfer protocol.
imsg input<Ptfg\0>got 4 characters	Remote sends ªPtfg.º
got Ptfg	Remote knows these protocols.
wmesg 'U' g	Want the ªgº protocol (dial-up serial line).
omsg <Ug>
Proto started g	Starting the ªgº protocol.
protocol g
root rhino (7/18-09:27-4187) OK (startup cufa 19200 baud)	Protocol startup message.
*** TOP ***  -  role=MASTER	Starting up, in master role.
wmesg 'H' 	Nothing to send; does the remote have anything?
rmesg - 'H' got HY
PROCESS: msg - HY
HUP:
wmesg 'H' Y
cntrl - 0	Nothing on the remote; shut down.
root rhino (7/18-09:27-4187) OK (conversation complete)	Termination message.
send OO 0,omsg <OOOOOO>	Cleanly shutting down.
imsg looking for SYNC<\20>
imsg input<   \10*"   \20>
imsg input<   \10*"   \20>
imsg input<   "*\10   \20>
imsg input<   "*\10   \20>
imsg input<OOOOOO\0>got 6 characters	Connection shutdown complete.