Axis Conversion Inspector

Temperature Axis Conversion
The X or Y axis can be converted from degrees Celsius or Fahrenheit to degrees Kelvin and vice versa.

PES Axis Conversion
This function converts the energy (X) axis of photo electron spectra depending on the excitation energy, from binding energy to kinetic energy and vice versa.

XRD Axis Conversion
This function converts the X axis of X-ray diffraction spectra depending on the X-ray wavelength, from 2Theta to d and vice versa.