NEXTSTEP for Intel Processors
Tested Compatible System

Title:	Advanced/ZE 100mhz with 4mb Video Option 
Last Updated:	September 22 1995
Effective Date:	September 22nd 1995
Tested with:		3.3

Product Vendor:
Workstation 2000: 
	W2000@CTS.COM or 1-800-A-STATION

Explanation of Compatibility Testing 
NEXTSTEP Compatible systems are tested by third parties using a test procedure developed by NeXT. NeXT approves the use of the "NEXTSTEP Compatible" designation for these systems based on the completeness of the test results submitted by these NeXT-trained 3rd parties.
 
For more detailed information on the NICE program, please refer to NeXTanswers document 1903_Compatible_Systems_Tested_With_NEXTSTEP.rtf

Note:	NeXT accepts no support responsibilities or liability whatsoever for any system authorized to use the "NEXTSTEP Compatible" designation, nor does NeXT represent that their test procedures or training--even if followed exactly by the 3rd party performing the test work--are in any way complete or exhaustive. Known or unknown errors may be present in configurations which are designated as "NEXTSTEP Compatible" which could adversely affect the operation of these systems. Support for compatible systems may be provided by the PC vendor or System integrator. 

Tested Components:
Workstation 2000 reports testing a system configuration consisting of the following components:
Summary information only. Contact Workstation 2000 for more specific configuration information

System CPU Board(s)
	CPU:		Intel Pentium, 100MHz
	RAM:		16mb min, 128MB maximum tested

SCSI Controller(s)
	Manufacturer:	ADAPTEC
	Model name:	2940
	Interface:		PCI

CD-ROM Drive(s)
	Manufacturer:	SONY
	Model name:	CDU
	Interface:		SCSI

Hard Drive(s)
	Manufacturer:	CONNER
	Size:		1GB

Graphics Adaptor(s)
	Manufacturer:	Diamond 
	Model name:	Stealth 64 PCI 4mb 
	Video RAM:	4mb
	RAM Type:	VRAM
	Interface:		PCI

Serial Port(s)
	Ports:	2
	UART:	16C550

Parallel Port(s)
	on-board, LPT1

Keyboard(s)
	Manufacturer:	NMB
	Model name:	RT101+
	Interface:		PS/2, PC/AT

Mice and Other Pointing Devices
	Manufacturer:	MICROSOFT
	Model name:	MOUSE PORT COMPAT. MOUSE
	Interface:		PS/2

LAN Adaptor(s)
	Manufacturer:	COGENT
	Model name:	EMASTER+
	Interface:		PCI
	Connectors:	BNC*,  TP*
	* Adaptor tested with this connector

Sound Card(s)
	Manufacturer:	CREATIVE TECHNOLOGY 
	Model name:	Sound Blaster 16 Value Edition
	Interface:		ISA 

Monitor(s)
	Manufacturer:		CTX 
	Model name:		GM
	Size:			17
	Max resolution:	1280X1024X72

Note that only the specific components listed were tested.

Setup and Installation
Hardware Setup:
	See above for individual setup instructions for each adaptor.

CMOS settings:
To Access:
F1
Settings:
Factory settings 

ECU settings (EISA-bus systems only):
NA 
	
Special installation instructions:

Driver settings:
Use Configure.app to load and configure the following drivers:
Display 
	DiamondStealth64DisplayDriver
Pointing Device
	PS2Mouse
Network 
	CogentEM960NetworkDriver
SCSI
	Adaptec2940SCSIDriver
Audio 
	SoundBlaster16
Other
	SerialPorts
	Floppy Disk 
	PS2Keyboard
	PCIBus
	EISABus
	ParallelPort
			
Known Problems
This is a NS bug in 3.3: This is an S3 graphics system, with these 
cards, must boot in verbose mode.

See Also:	(None)