Calculation Inspector

Subtract & Add Buffer
With this function buffers (specified by reference numbers from the File Inspector) can be added to or subtracted from each other, depending on the selection within the Mode radio button.

Data Reduction
Sometimes it is useful to reduce a large number of datapoints which consist mainly of noise to a more practical amount of points. This function takes n points (n is specified in the Factor  field), builds the average, and replaces the n points with the new one.

Integrate
This function calculates the integral between the X min and X max value, multiplicates and divides it by the given factors, and writes the result to the comment fields in the File Inspector. 

The Result Mode radio button selects the output format.
e.g.	Short Form:	Int=10.0
	LongForm:	Int(2.0,7.0)=10.0

Clicking the Make % button calculates the relative values of the integrals for all selected buffers in which an integral entry (as above) appears and appends the percentage to the integral entry.

Calculations
Three kinds of calculations are possible:

1. 	(x,y)  =  Value  (+,-,*,/)  (x,y)

2. 	(x,y)  =  (x,y)  (+,-,*,/)  Value

3. 	(x,y)  =  (Log,Log10,Exp,Exp10, Sin,Cos,^2,Sqrt) (x,y)

These calculations effect all selected buffers.