AMD PCnet-32 Ethernet Adapter
¬

¬Network Devices
This VL-bus and PCI bus device driver is designed to run on an Intel-based computer running OPENSTEPä for Mach Release 4.0. In PCI implementations it automatically detects the target adapter. 

Supported Hardware: 

This driver supports AMD PCnet-32 based add on cards and motherboard implementations. It supports Am79C965 (VL-bus), Am79C970 (PCI) and Am79C974 (PCI) chipsets.

Installation and Configuration Steps for PCI chipset(s):
1. 	Install the adapter in the system (if necessary).
2. 	Log in as root and run Configure.  
3.	Click on the Network Devices icon at the top of Configure's "Summary of Devices" window.  In the Add Network Devices panel that opens, select the radio button labeled "Show Drivers for Detected Devices" if it is not already highlighted.  
4.	Select "AMD PCnet-32 PCI Ethernet Adapter" from the list, and click Add. 
5. 	Click Done, then click Save, then quit Configure.

Installation and Configuration Steps for VL-bus chipset:
1. 	Install the adapter in the system (if necessary).
2. 	Log in as root and run Configure.  
3.	Click on the Network Devices icon at the top of Configure's "Summary of Devices" window.  In the Add Network Devices panel that opens, select the radio button labeled "Show All Installed Drivers" if it is not already highlighted.  
4.	Select "AMD PCnet-32 Ethernet Adapter" from the list, and click Add. 
5. 	Click Done, then click Save, then quit Configure.

¬
	
See also

·	"Add a Device" in Configure's on-line help.

·	See NeXTanswer 1824 for general information on installing and configuring device drivers.