Modify Register reg.|IP|SP|SR,value

Allows you to change the contents of a CPU register. You must identify the register and follow it with the new contents.