Display Code location

Allows you to view the disassembled IBot program in memory. You must identify the location to begin the listing (for example, IP for the current instruction pointer).