*
* Printer Definition for IBM's ProPrinter
*
TOPMARGIN 0
BOTMARGIN 0
LINELEN 80
LINESPAGE 66
*
DOT			* DOT LETTER LASER
COMPON 15		* set compressed print
COMPOFF 18
FFEED 12		* Form Feed Character
EXPAND 14		* SET EXPANDED PRINT
EXPANDOFF
MICSPACE 27 65 9	 * SET MICRO SPACING to n 72nds of an inch
FORMLENL 27 67 66	  * set form length in lines  66 = 66 lines
FORMLENI 27 67 0 11	 * Set form length in inches 11 = inches
EMPH 27 69
EMPHOFF 27 70
DOUBLE 27 71		   * double strike (nlq) printing
DOUBLEOFF 27 72
NLQ 27 73 2
NLQOFF 27 73 0
DLFONT 27 73 4		 * Download font off
DLFONTOFF 27 73 0
PERFSKIP  27 78 4	 * set number lines to skip over perfs (4)
PERFSKIPOFF 27 79
ONEDIR 27 85 1		 * print in only 1 direction
ONEDIROFF 27 85 0
8LPI 27 48
6LPI 27 50
CHARSET 27 54		 * Select char set 2   27 55 = char set 1
CHARSETOFF 27 55
12CPI 27 58		 * 12 characters per inch
12CPIOFF 18
