*
* Printer Definition for HP LASER PRINTER FAMILY
*
*--------------------------------------------------------------------
* The following options are set immediately.  They are not activated
* by parameters.
*--------------------------------------------------------------------
LASER                   * LASER PRINTER
TOPMARGIN 4
BOTMARGIN 4
LINELEN 80
LINESPAGE 66
*MICSPACE 27 65 9         * SET MICRO SPACING to n 72nds of an inch
*FORMLENL 27 38 108 66 80  * set form length in lines  66 = 66 lines
FFEED 12                * Form Feed Character
*--------------------------------------------------------------------
* The following parameters are activated by parameters
*--------------------------------------------------------------------
EMPH 27 40 115 51 66
EMPHOFF 27 40 115 48 66
PERFSKIP  27 38 108 49 76 * set number lines to skip over perfs (4)
PERFSKIPOFF 27 38 108 48 76
8LPI 27 38 108 56 68
6LPI 27 38 108 54 68
COMPON 27 40 115 49 54 46 54 72     * 16.66 CPI
COMPOFF 27 40 115 49 48 72        * 10 CPI
*12CPI 27 40 115 49 50 72         * 12 characters per inch
*12CPIOFF 27 40 115 49 48 72      * 10 CPI
*
* FUTURES ------------------------------------------------------
*
PROPORTIONAL 27 40 115 49 80
PROPORTIONALOFF 27 40 115 48 80   * FIXED SPACING

* ORIENTATION
PORTRAIT 27 38 108 48 79
LANDSCAPE 27 38 108 49 79

* SYMBOL SET
ROMAN8 27 40 56 85
USASCII 27 40 48 85
ROMANX 27 40 48 69
LEGAL 27 40 49 85
LINEDRAW 27 40 48 66
PIFONT 27 40 49 53 85
PIFONTA 27 40 50 81

* POINT SIZE
POINT7  27 40 115 55 86
POINT8  27 40 115 56 86
POINT85 27 40 115 55 46 53 86
POINT10 27 40 115 49 48 86
POINT12 27 40 115 49 50 86
POINT14 27 40 115 49 52 46 52 86

* TYPEFACE
COURIER 27 40 115 51 84
LINEPRINTER 27 40 115 48 84
HELV 27 40 115 52 84
TIMESROMAN 27 40 115 53 84
PRESTIGEELITE 27 40 115 56 84
GOTHIC 27 40 115 54 84
