Has built-in RGB display that is similar to the “Basic 14” Color Display” in the above display list.  The LC 575 display has a dot pitch of .26 mm with a vertical refresh rate of 67Hz.

Comes with 512 KB of VRAM in the form of two 256KB SIMMs.

A 1MB VRAM configuration is achieved by replacing the two 256KB VRAM SIMMs with 512KB SIMMs.