12.1” (diagonal) active-matrix color SVGA LCD Display.

Resolution is 800 x 600 pixels.

Supports mirrored 8-bit (256 colors) video output to 21” monitor in SVGA mode.  Supports mirrored 16-bit (thousands of colors) video output on smaller monitors in SVGA mode.