"A) SuperK Xmodem Single [Checksum - 80% eff.]
",5,S,8,,,128,,0.8,,4=F,"SUPERK.COM p[PORT#] s[BAUD] n[NODE] dS tx f[FILE]","SUPERK.COM  p[PORT#] s[BAUD] n[NODE] dR tx f[FILE]"
"1) SuperK Xmodem Batch [Checksum - 80% eff.]
",5,S,8,,B,128,,0.8,,4=F,"SUPERK.COM p[PORT#] s[BAUD] n[NODE] dS r txb f[FILE]","SUPERK.COM  p[PORT#] s[BAUD] n[NODE] dR r txb f[FILE]"
"B) SuperK Xmodem CRC Single [CRC - 80% eff.]
",5,S,8,,,128,,0.8,,4=F,"SUPERK.COM p[PORT#] s[BAUD] n[NODE] dS tc f[FILE]","SUPERK.COM  p[PORT#] s[BAUD] n[NODE] dR tc f[FILE]"
"2) SuperK Xmodem CRC Batch [CRC - 80% eff.]
",5,S,8,,B,128,,0.8,,4=F,"SUPERK.COM p[PORT#] s[BAUD] n[NODE] dS r tcb f[FILE]","SUPERK.COM  p[PORT#] s[BAUD] n[NODE] dR r tcb f[FILE]"
"C) SuperK Ymodem Single [1k Xmodem - 87% eff.]
",5,S,8,,,1024,,0.87,,4=F,"SUPERK.COM p[PORT#] s[BAUD] n[NODE] dS ty f[FILE]","SUPERK.COM  p[PORT#] s[BAUD] n[NODE] dR ty f[FILE]"
"3) SuperK Ymodem Batch [1k Xmodem - 87% eff.]
",5,S,8,,B,1024,,0.87,,4=F,"SUPERK.COM p[PORT#] s[BAUD] n[NODE] dS r tyb f[FILE]","SUPERK.COM  p[PORT#] s[BAUD] n[NODE] dR r tyb f[FILE]"
"D) SuperK WXmodem Single (*ok w/WXMODEM) [Sliding Window - 87% eff.]
",5,S,8,,,128,,0.87,,4=F,"SUPERK.COM p[PORT#] s[BAUD] n[NODE] dS tw f[FILE]","SUPERK.COM  p[PORT#] s[BAUD] n[NODE] dR tw f[FILE]"
"4) SuperK WXmodem Batch [Sliding Window - 87% eff.]
",5,S,8,,B,128,,0.87,,4=F,"SUPERK.COM p[PORT#] s[BAUD] n[NODE] dS r twb f[FILE]","SUPERK.COM  p[PORT#] s[BAUD] n[NODE] dR r twb f[FILE]"
"E) SuperK K9Xmodem Single [ 90% eff.]
",5,S,8,,,0,,0.90,,4=F,"SUPERK.COM p[PORT#] s[BAUD] n[NODE] dS tk f[FILE]","SUPERK.COM  p[PORT#] s[BAUD] n[NODE] dR tk f[FILE]"
"5) SuperK K9Xmodem Batch [ 90% eff.]
",5,S,8,,B,0,,0.90,,4=F,"SUPERK.COM p[PORT#] s[BAUD] n[NODE] dS r tkb f[FILE]","SUPERK.COM  p[PORT#] s[BAUD] n[NODE] dR r tkb f[FILE]"
"F) Super8K Single (fast as ZMODEM) [8k Packet - 92% eff.]
",5,S,8,,,0,,0.92,,4=F,"SUPERK.COM p[PORT#] s[BAUD] n[NODE] dS ts f[FILE]","SUPERK.COM  p[PORT#] s[BAUD] n[NODE] dR ts f[FILE]"
"6) Super8K Batch (fast as ZMODEM) [8k Packet - 92% eff.]
",5,S,8,,B,0,,0.92,,4=F,"SUPERK.COM p[PORT#] s[BAUD] n[NODE] dS tsb r f[FILE]","SUPERK.COM  p[PORT#] s[BAUD] n[NODE] dR r tsb f[FILE]"
"G) Jmodem 8k Single [ Variable Packet Size - 87% eff.]
",5,S,8,,,0,,0.87,,4=F,"JBATCH.COM p[PORT#] s[BAUD] n[NODE] dS b f[FILE]","JBATCH.COM  p[PORT#] s[BAUD] n[NODE] b dR f[FILE]"
"7) Jmodem 8k Batch [ Variable Packet Size - 87% eff.]
",5,S,8,,B,0,,0.87,,4=F,"JBATCH.COM p[PORT#] s[BAUD] n[NODE] dS f[FILE]","JBATCH.COM  p[PORT#] s[BAUD] n[NODE] r dR f[FILE]"
"H) DSZ Ymodem-G Single [ 90% eff.]
",5,S,8,R,,1024,F,0.9,,1=E,"DSZ.COM port [PORT#] speed [BAUD] ha on -g sb [FILE]","DSZ.COM port [PORT#] speed [BAUD] ha slow -g rb [FILE]"
"K) Kermit Single [ PCKERMIT - 78% eff.]
",5,S,,,,128,F,0.78,,,"PCKERMIT.EXE -s [FILE] -l [PORT] -c -b [BAUD] -p [PARITY] -m 31","PCKERMIT.EXE -r -a [FILE] -l [PORT] -c -b [BAUD] -p [PARITY] -m 31"
"M) Megalink Batch (up to 50 files) [ 1024K Packet - 95% eff. ] 
",5,S,8,,B,1024,F,0.95,,1=E,"MLINK11.COM port [PORT#] speed [BAUD] SM [FILE]","MLINK11.COM port [PORT#] speed [BAUD] RM [FILE]" 
"P) Standard CRC Xmodem Single [ 78% eff.]
",5,IC,8,,,128,,0.78,,,,
"X) Standard Xmodem [ 78% eff.]
",5,IX,8,,,128,,0.78,,,,
"Y) Standard Ymodem [ 87% eff.]
",5,IY,8,,,1024,,0.87,,,,
"8) DSZ Ymodem Batch [ 90% eff.]
",5,S,8,,B,1024,F,0.90,,1=E,"DSZ.COM port [PORT#] speed [BAUD] sb -k [FILE]","DSZ.COM port [PORT#] speed [BAUD] rb -p [FILE]"
"Z) DSZ Zmodem Single [ 95% eff.]
",5,S,8,,,1024,F,0.95,,1=E,"DSZ.COM port [PORT#] speed [BAUD] pB4096 ha both D sz -r -n -b -e -w [FILE]","DSZ.COM port [PORT#] speed [BAUD] pB4096 ha both D rz -r -n -b -e -w [FILE]"
"9) DSZ Zmodem Batch [ 95% eff.]
",5,S,8,,B,1024,F,0.95,,1=E,"DSZ.COM port [PORT#] speed [BAUD] pB4096 ha both D sz -r -b -n -e -w [FILE]","DSZ.COM port [PORT#] speed [BAUD] pB4096 ha both D rz -r -b -n -e -w [FILE]"
"N) None - Cancel 

Select Protocol",4,IN,,,,,,,,,,

