6. Switch to the Top view and select the extruded "strut" you've just created, then press [command] R to bring up the Replicate dialogue box. Set the Axis offset boxes (the top ones) to X=0.0, Y=0.0 and Z=-10. Then set the Repetitions box to 9. Click OK, and then press [command] G to group the struts together.