3. Use the Cylinder Primitive tool to enter a cylinder in the modelling window. Yet again using the Transform dialogue box, set the cylinder's dimensions to X=6.0, Y=6.0 and Z=24 metres. Position the cylinder between the two spheres.