Modem Information

INIT String -  This is the default INIT string used if a BOSS does not have a custom string attached to it.    Note: This only works if the Copernicus - Call Application or the Tabby - TabbyNet Application is being used as the mailer.

Modem Type - This identifies the type of modem you are using.  This is for use with future versions of TOMCAT mailer.

Baud - Check the box that indicates the maximum baud rate that the modem attached to this system can handle.  (300, 1200, 2400, 9600, 19200, 38400, 56800).

Tone Dial - Check this box if a touch tone phone line is being used.  This is only used with Copernicus/Tabbynet/TomCat Modules.

Modem Port - Check this box if communication is to be performed through the modem port.  Otherwise, the printer port will be used.  This is only used with Copernicus/Tabbynet/TomCat Modules

MultiFinder - Check this box if running under MultiFinder or System 7.  This is only used with Copernicus/Tabbynet/TomCat Modules.

Lock Port - Check this box if the baud rate should be locked on the local end.  This is only used with Copernicus/Tabbynet/TomCat Modules.
  
Save Button - Will save the information in the current dialog box as new default information.

Cancel Button - will revert to the old settings, as they were prior to entering this dialog box.