Spec Sheets

Model            6100/60         7100/66         8100/80
 
Processor        PPC601          PPC601          PPC601
     Speed       60mhz           66mhz           80mhz
     Cache       Optional        Optional        256k standard
 
Performance                      25% faster      200% faster
     Native      2-4x 68040/33   than 6100/60    than 6100/60
     Emulated    fast 030-040
 
RAM              8MB Standard    8MB Standard    8MB Standard
     DRAM exp.   72MB            136MB           264MB
     SIMM Slots  2               4               8
 
Expansion Slots  One 7" NuBus    3 Full Size     3 Full Size
                                 NuBus           NuBus
Storage
     Standard    160 to 250 MB   250 to 500 MB   250MB to 1GB
     Floppy      1.4MB w/DMA     1.4MB w/DMA     1.4MB w/DMA
     CD-ROM      Optional        Optional        Optional
 
Video
     DRAM video  Standard        Standard        Standard
     VRAM                        1MB Standard    2MB Standard
     VRAM exp.                   2MB             4MB
Standard Support 1 Monitor       2 Monitors      2 Monitors
 
SCSI             High-speed      High-speed      High-speed
                 asynch.         asynch.         asynch.
                                                 Dual SCSI
                                                 channels
 
Networking   Ethernet on-board w/DMA channel, AAUI connector
 
Other Built-ins     
     16-bit audio stereo in/out with DMA
     2 Serial ports-LocalTalk and GeoPort compatible,with DMA
     channel Apple Desktop Bus (ADB for input devices)

AV Models 6100/66AV, 7100/66AV, 8100/80AV
     Video-in  NTSC,PAL,SECAM
               video in resizeable window
               Frame and video capture
 
     Video-out NTSC,PAL
     VRAM      2MB standard, not expandable
     Interface S-video for video in/out
               Composite (RCA) adapters included
 
Software
     System 7.1.2 Macintosh operating system with AppleScript
          PC Exchange & QuickTime.
     PlainTalk text-to-speech and speech recognition software
     MS-DOS/Windows 3.1 with Insignia Solutions SoftWindows(TM)
          software
 
Other
     SIMM      72-pin, 80ns or faster, installed in pairs
     CD-ROM    AppleCD 300i
     Power     100-240 volts, 50-60 Hz
               EnergyStar compliant (7100/66, 8100/80)