Test Network

You may select a network (or a range of networks) to be tested. Choose Test Network from the MacPing menu, or Test AppleTalk from the Network pop-up menu. Type the desired network number and click OK.

To enter a network range, type the two numbers separated by a hyphen (-). MacPing will discover devices on the network number(s) and update the Zone pop-up menu properly. 

If you know the network address of a particular device that you want to test, you may enter that address (in the form network/node).  MacPing will test that address along with the other devices on that network.

Note: You can enter and display numbers in octal, decimal, or hexadecimal. These settings then apply throughout the program. 

Note: You can use this feature as a number base converter. Type the number to be converted and select a new base.