*********************************************************

In an effort to keep up to date with all machine types, I've decided to convert BugOff to a fat binary format.  This allows it to run in native mode on both 680x0 and Power PC based machines.  Since this package runs continously in the background, I felt it was necessary to convert it on Power PC based machines as to prevent the system from running in emulation mode.

The fat binary increases the size of the overall application significantly.  If this increased size is a problem for some users I will be more than happy to release either a 680x0 or Power PC only copy of the program.  If you require the reduced size application please notify me via Email.  You will save approximately 150K by using the reduced version.  

There's an indicator to notify the user which mode BugOff is executing.  If the status window title is "BugOff" it's in 680x0 mode. If the title is "BugOff!" you're running in Power PC native mode.

*********************************************************