Release 3.2  Copyright ã1993 by NeXT Computer, Inc.  All Rights Reserved.

3.2 Release Notes: 
InstallTablet

New Features

The following features have been added to InstallTablet since Release 2.0.

·	InstallTablet has been enhanced in NEXTSTEP Release 3 to support a wider range of WACOM tablets. This version of the tablet driver supports the following WACOM tablets: SD-210, SD-310, SD-311, SD-312, SD-320, SD-321, SD-322, SD-420, SD-421, SD-422, SD-510B, and SD-510C. The standard pen and puck for these tablets implement both left and right mouse buttons. The pressure pen implements only the left mouse button. 

·	The tablet driver now supports WACOM pressure sensitive tablets and allows applications that are pressure-aware to read pressure values emitted by the pressure pen. To start using the pressure pen, first turn on the Pressure Pen switch to inform the tablet driver. In this mode you should only use the pressure pen±±using the puck or standard pen won't work properly. In normal mode the pressure pen won't work properly. To switch back to using the normal puck or pen, first turn off the Pressure Pen switch. You should switch pressure modes using the mouse, not the tablet.

·	Be sure that you WACOM tablet is set to these factory default switch settings:

¬

·	If you're having problems with a WACOM tablet, it sometimes helps to click Remove, reset the tablet (or power it off and on), and click Install.