1957 Options                                QTY      LIST
  Base Corvette Convertible                  6,339  $3,176.32
  Heater                                     5,373     118.40
  AM Radio, signal seeking                   3,635     199.10
  Parking Brake Alarm                        1,873       5.40
  Courtesy lights                            2,489       8.65
  Windshield Washers                         2,555      11 85
  Wheels, 15x5.5(5)                             51      15.10
  Whitewall Tires 6.70x15                    5,019      31.60
  3-Spd Man. Transmission close ratio        2,886      00.00
  Powerglide Automatic Transmission          1,393     188.30
  Auxiliary Hardtop                          4,055     215 20
  Power Windows                                379      59.20
  Two-Tone Paint Combination                 2,797      19.40
  Power Operating Folding Top                1,336     139.90
  Positraction Rear Axle. 3.70:1               327      48.45
  Positraction Rear Axle. 4.11:1             1,772      48.45
  Positraction Rear Axle. 4.56:1                        48.45
  Heavy Duty Racing Suspension                  51     780.10
  4-Speed Manual Transmission                  664     188.30
  283ci/245hp Engine (2x4 carburetors)       2,045     150.65
  283ci/270hp Engine (2x4 carburetors)       1,621     182.95
  283ci/250hp Engine (fuel injection)          182     484.20
  283ci/283hp Engine (fuel injection)          713     484.20
  283ci/250hp Engine {fuel injection)          102     484 20
  283ci/283hp Engine (fuel injection)           43     726.30
   (includes tachometer & fresh air intake)