Mallett 435 Features

435 Horsepower LS-1 V-8 
372 Cubic Inches (6.1 Liters) 
Billet Steel Crankshaft 
Billet Steel Connecting Rods 
Forged Aluminum Lightweight Pistons 
Custom Mallett-Spec. Performance Cam 
Custom 4340 Chromoly Steel Pushrods 
Custom Valve Springs & Lightweight Retainers 
Custom Carbon-Fiber Intake Manifold 
Carbon-Fiber Coil/Rocker Covers 
2.50" Stainless & Carbon-Fiber Mufflers 
Hand Assembly & Performance Testing 

Competition-Tuned Suspension 
Z-51 Springs 
Penske/Mallett Double Adjustable Indy-Style Shocks 
Mallett-Designed Competition-Rate Front Tubular Sway Bar 
17x9.5 Front & 17x11 Rear Forged Aluminum Wheels 
275/40/17 Front & 315/35/17 Rear, Goodyear Eagle ZR-S Tires 
Lowered Ride Height 

Interior/Functional 
Carbon-Fiber Dash and Console Trim 
Serial Number Plaque 
Custom Billet Aluminum Shifter 
Custom Embroidery on Seats 

Appearance 
Mallett-Specific body Graphics 
Mallett Exclusive Forged Alloy Wheels 

Special Features 
Limited Lifetime Membership in the National Corvette Museum (NCM) 
Archival Display of Owner's Name and Vehicle Serial Number at NCM 
Mallett Cars Newsletter 
Limited Production (100 cars in 1998) 

Performance*:
0-60: 4.1 seconds
Quarter Mile: 11.996 @ 117.38 mph
Top Speed: 190+ mph
Skid Pad: 1.0 g

*All performance numbers achieved on stock Mallett 435-issue Goodyear ZR-S 
tires, through the catalytic converters, with full exhaust and accessories, sway bars
attached, no track-bite compound used on the track or tires.