.0 The mailbox (Overview)

This programme allows several different levels of remote access. For you it allows you to read and write data. We know this is not a new idea, but what is new is that we offer it in one programme. By this stage you maybe beginning to understand  that CoMa is truly a "communication manager".

With the integrated Z-modem you can download and upload data, and using the "mail" function messages can be left for other people in the mailbox.

With the x-modem you are able to send a new firmware into your modem.

The inbuilt terminalprogramm alows you to connect to any mailbox or to configure your modem by using the AT-commands.

Password in CoMa

As we said there is several different levels of access, and these are:

* The User

You can set up for yourself with your own "supervisor" password full access to all levels in your computer.

* Guests

Remote access can be given to "common" users via the password "guests". They are restricted to the allocated folder, but this folder may contain several sub-folders.

* Friends

You can set up a separate folder for a person of your choice, to which they have their own  password. Again, access is restricted to this single folder, but it may contain sub-folders. 

Password in CoMa Professional 

This function is greatly extended in CoMa Professional in which you can create

*unlimited "friends" folders 

with unlimited passwords. The mailbox is fully useable in this version for business and personal use.

The terminalprogramm

You don´t need to use any other programm to configure your modem or to connect to any mailbox. Just use CoMa´s own terminalprogramm.

For the receive from a mailbox (download) you can use the built-in Z-Modem.

If you want to send something to a mailbox you can choose between two functions

   * Z-Modem Upload 
   * ASCII Upload 
    * X-Modem Upload (for firmware upload into a modem)

You can use drag & drop here. Just drag a file on the terminal window and drop it there. CoMa starts at once to send this file with Z-Modem.