--------------------------------------------------------------------------
--INSBCIR.DEF
--This is the input file to BLDF that makes a .HLP file for the 
--UPL 'INSert BCIRcle' command.


--Type 'BLDF INSBCIR.DEF' to create help file named INSBCIR.HLP; this file
--should be kept in the same directory as INSBCIR.UCD.

--------------------------------------------------------------------------

--This first section just sets up a temporary modifiers file that is
--only used by the BLDF utility when it is processing the the HELP section
--below.  Note that these modifiers are set up the same way the modifiers
--are set up in the INSBCIR UPL program.

BEGIN MOD
FILE NEW INSBCIR.MOD
 
MOD 1 HOLEDia           R
MOD 1 CIRDia            R
MOD 1 ABegin            R
MOD 1 AIncrement        R
MOD 1 Nholes            I
MOD 1 COLor             I
MOD 1 FONt              I
MOD 1 LAYer             I

END MOD

--Help section----------------------------------------------------------------

Begin Help                      --Must use this command at beginning of file.
File INSBCIR.HLP                --Compiled output filename.  Can be any name.
File Modifiers INSBCIR.MOD      --Compiled modifier processor name. (Note that
                                --this file (INSBCIR.MOD) was generated above
                                --in the MOD section of this file.      

-------------------------------------------------------------------------------

VNP 1 2

                           INSert BCIRcle

        This command is used to insert bolt circle patterns.  You
        can specify the circle diameter and the diameter of the
        holes around the circle.


   Press 'More' key for more detailed help on individual modifiers
@

Help 2  3 4 5 6 7 8

  The following modifiers are availiable for INSert BCIRcle:

        F1 - HOLEDia

        F2 - CIRDia

        F3 - ABegin

        F4 - AIncrement

        F5 - Nholes

        F6 - COLor, FONt, LAYer

  for help on a specific modifier, press the specified Function key
@

Help 3          --used by Help 2, [F1]

        The HOLEDia specifices the diameter of the holes put in
        around the bolt circle.
@

Help 4          --used by Help 2, [F2]

        The CIRDia specifies the diameter of the circle that the
        holes will be placed on.
@

Help 5  8       --used by Help 2, [F3]

        The ABegin specifies the begining angle to start the holes.
        The 3 o'clock position is 0 degrees and 12 o'clock is 90.
@

Help 6          --used by Help 2, [F4]

        The AIncrement specifies the angle between each hole.
@

Help 7          --used by Help 2, [F5]

        The Nholes specifies the number of holes to make on each circle.
@

Help 8          --used by Help 2, [F6]

        The COLor, FONT and LAYer modifiers are used to set the display
        characteristics of the inserted circles.  The inital default
        values are:

        COLor  - current GCD default color
        FONT   - style 2
        LAYer  - layer 256
@

ModIndex 1 2     --index 1 is for UPL defined modifiers, 2 is for 'more' help

Modifiers Default

        There are several modifiers that can be selected to set such
        things as the hole diameters, the circle diameter, begining
        and increment angles, number of holes to put in and the
        characteristics of the circles inserted such as color, font and
        layer.

        Press 'More' key for more detailed help on the individual
        modifiers  or  press the 'Previous' key for general help with
        the INSert BCIRcle command.
@

GetData 1

        You are being prompted to enter the location(s) of the
        centers of the bolt circle patterns you want to insert.
        You can insert up to 400 bolt circle patterns at a time.

        If you need to change some of the modifers before or after
        you have inserted some bolt circles, you can enter a ':' to
        return you to the modifier processor section.
@

End Help
End
