Supra Modem CCL Files for OSX 
©April 2001 Readme File 
Diamond Multimedia Systems, Inc. /  A Division of Sonic|blue Inc. 
All Rights Reserved
••••••••••••••••••••••••••••••••••••••••••••
Contents
1.  Content Folders
2.  Installation and Use
3.  Known Limitations / Issues
••••••••••••••••••••••••••••••••••••••••••••

1. Content Folders

OSX_Serial Modem CCLs
-----------------------
Serial Standard CCLs
SerialTroubleshooting CCLs
Legacy Modems
OSX_Serial Modem CCL ReadMe
OSX_Serial Modem CCL ReadMe.rtf

OSX_SUP 2780 USB-CCLS
-----------------------
USB Standard CCLs
USB Troubleshooting CCLs
OSX_SUP 2780-CCLS README
OSX_SUP 2780 CCLS README.rtf

2.  Installation and Use

To use these files with OSX, you will need to move these files into the Modem Scripts folder, inside the Library folder, within the root directory of the hard drive.  A restart is normally required.  Go to System Properties ->Network-> Modem , select the proper script / CCL for your hardware.

3.  Known Limitations / Issues
If you use a USB script with a serial modem, your modem may not initialize properly.  Also, if you use a serial script with the SupraExpress USB, the modem may not initialize.

Supra Cable Test is not supported with the USB modem.

Supra 56 for PowerMac will set the serial port speed to 115200 - a speed non-PowerPC based Macs are not capable of. 

RLW041901