This control surface is located on the fin. It is used to control the planeÕs yaw.