3.

You will Need

¥ IsopropylAlcohol -At least 90% strength ¥ Lint-Free Cloth ¥ 3M Cleaning Kit (77-9803-8546-0) BeforeYou Begin

Turn off the Rainbow proofer and the computer, then remove the base cassette tray and ink ribbon tray from the proofer. Warning: Alcohol is highly flammable. When using alcohol, avoid sparks, flames, and other combustion sources. Caution: Do NOT force the cover open! Caution: Avoid touching the ink ribbon with isopropyl alcohol! Important: When cleaning the thermal head, touch and hold your free hand to any metal portion of the proofer prior to and during cleaning. Important: Follow the cleaning procedure in order.Allow the proofer to dry at least 10 minutes prior to performing a Self-Print Test, and one hour prior to making critical color proofs.

Inside of Proofer Cover

Use lint-free cloth dampened with isopropyl alcohol

. 1. Clamp Bar

Use cleaning tool dampened with isopropyl alcohol. Clean each clamp. 2.