A2PS ( 1L ) MISC. REFERENCE MANUAL PAGES A2PS ( 1L )

NAME

a2ps – formats an ascii file for printing in a postscript printer; very nice and compact format for program listings. S SYNOPSI

a2ps [ -b ] [ -f ] [ -i ] [ -n ] [ -n{bfinrv} ] [ -r ] [ -v ] [ file1 ] [ file2 ] [...] DESCRIPTION a2ps formats files "file1", "file2", ... for printing in a postscript printer; if no file is given, a2ps reads , b from the standard input. Format used is very nice and compact: two pages on each physical page orders surrounding pages, headers with useful information (page number, printing date, file name), line O numbering, etc. Very useful to archive listings of programs.

ptions offered by a2ps are the following: -b Force printing binary files. By default, binary files printing is stopped before second page - (see -nb option).

f Fold lines too large to be printed inside the borders (default option). Max size is actually 86 - characters.

i Interpret TAB, BS and FF characters (default option). TAB is replaced by enough spaces to - reach next tab stop while BS and FF have their meanings.

n Output lines are preceded by line numbers, numbered sequentially from 1 (default option). e -nb Don’t print binary files. To detect such a file we make use of a very simple heuristic: if th first page of the file contains at less 75% of non-printing characters, it’s a binary file. First - page is always printed.

nf Cut lines too large (don’t fold). -ni Don’t interpret TAB, BS and FF characters. They will be printed according to -v option.

- -nn Don’t number output lines. nr Sheet numbering (see -r option) must be continue for all files (don’t reset on new file).

- -nv Replace non-printing characters by a space. r Reset sheet numbering for each new file (default option). Sheet numbering is used to number f physical pages (sheets printed) and is placed in the bottom of each physical page. It differs rom page numbering: logical pages of file been printed. . -v Replace non-printing characters so that they are lisible and easy to identify (default option) Control characters (ascii codes lower than 0x20) are printed like ^X for ctrl-x; the delete a character (hex 0x3f) is printed as ^?. Non ascii characters (with the high bit set) are printed s M- (for meta) followed by the character of the low 7 bits. TAB, BS and FF are handled

USAGE like non-printing characters if -ni option was taked.

a2ps sends formatted file to standard output. User could redirect this output to a file or pipe it directly to a print command, like lpr in UNIX:

a2ps file1 > file2 l D a2ps file1 | lpr - on’t forget -l option in last line, if you want that lpr interprets your postscript program. t f This filter must be used only with text files. Avoid specially output from TeX, troff or any other tex ormatter.

Sun Release 4.0 Last change: November 29 1988 1

)

S

A2PS ( 1L ) MISC. REFERENCE MANUAL PAGES A2PS ( 1L

EE ALSO pprps(1L) tgrind(1) lpr(1)

AUTHORS Evan Kirshenbaum (evan@csli) for the initial version. .

S

Miguel Santana (miguel@imag.imag.fr) for 2.0 version

un Release 4.0 Last change: November 29 1988 2