NOTE  This is the disk definition file for the 22NICE diskette
NOTE  utilities.  Refer to the 22DISK documentation for details.

BEGIN
  S8 Generic SSSD 8"
DENSITY
  FM,LOW
CYLINDERS
  77
SIDES
  1
SECTORS
  26,128
SIDE1 0
  1,7,13,19,25,5,11,
  17,23,3,9,15,21,2,
  8,14,20,26,6,12,18,
  24,4,10,16,22
BSH 3  BLM 7  EXM 0  DSM 242  DRM 63  AL0 11000000b AL1 00h  OFS 2
END

BEGIN
  O1 Osborne SSDD 5.25"
DENSITY
  MFM,LOW
CYLINDERS
  40
SIDES
  1
SKEW
  3
SECTORS
  5,1024
SIDE1
  0 1,2,3,4,5
BSH 3  BLM 7  EXM 0  DSM 180  DRM 63 AL0 11000000b AL1 0  OFS 3
END

BEGIN
  K1 Kaypro 2X/4X DSDD 5.25"
DENSITY
  MFM,LOW
CYLINDERS
  40
SIDES
  2
SKEW
  3
SECTORS
  10,512
SIDE1
  0  0,1,2,3,4,5,6,7,8,9
SIDE2
  0 10,11,12,13,14,15,16,17,18,19
BSH 4  BLM 15  EXM 1  DSM 200  DRM 63 AL0 11000000b AL1 0  OFS 1
END

BEGIN
  M1 Morrow MD1 SSDD 5.25"
DENSITY
  MFM,LOW
CYLINDERS
  40
SIDES
  1
SECTORS
  5,1024
SIDE1
  0 1,4,2,5,3
BSH 4  BLM 15  EXM 1  DSM 95  DRM 127 AL0 11000000b AL1 0  OFS 2
END

BEGIN
  M2 Morrow MD1 DSDD
DENSITY
  MFM,LOW
CYLINDERS
  40
SIDES
 2
SECTORS
  5,1024
SIDE1
  0 1,4,2,5,3
SIDE2
  1 1,4,2,5,3
BSH 4  BLM 15  EXM 1  DSM 194  DRM 191	AL0 11100000b  AL1 0  OFS 2
END

BEGIN
  A1 Actrix SSDD 5.25"
DENSITY
  MFM,LOW
CYLINDERS
  40
SIDES
  1
SECTORS
  9,512
SIDE1
  0 1,4,7,2,5,8,3,6,9
BSH 3  BLM 7  EXM 0  DSM 216  DRM 63 AL0 11000000b AL1 0  OFS 2
END

BEGIN
  H1 Heath SSSD
DENSITY
  FM,LOW
CYLINDERS
  40
SIDES
  1
SECTORS
 10,256
SIDE1
 0 1,2,3,4,5,6,7,8,9,10
BSH 3  BLM 7  EXM 0  DSM 91  DRM 63  AL0 11000000b  AL1 0  OFS 3
END

BEGIN
  H1 Heath SSDD - Magnolia CP/M
DENSITY
  MFM,LOW
CYLINDERS
 40
SIDES
 1
SECTORS
 9,512
SIDE1
 0 1,2,3,4,5,6,7,8,9
SKEW
 3
BSH 4  BLM 15  EXM 1  DSM 82  DRM 95  AL0 11000000b  AL1 0  OFS 3
END

BEGIN
  I1 IBM PC CP/M 86 SSDD
DENSITY
  MFM,LOW
CYLINDERS
  40
SIDES
  1
SECTORS
  8,512
SIDE1
  0 1,2,3,4,5,6,7,8
SKEW
  2
BSH 4  BLM 15  EXM 1  DSM 78  DRM 63  AL0 10000000b  AL1 0  OFS 1
END
