Sound and Music

Amiga Mail

Page VI - 7 Creating Virtual Voices with Amiga Audio

;/* interplay.c -- execute me to compile me
lc -b1 -cfist -v -j73 interplay.c
blink FROM lc:/lib/c.o + interplay.o TO interplay LIBRARY
lc:lib/lc.lib+lib:amiga.lib
quit
*/

/* Interlay.c - Run from Shell (CLI) only.  Given two file names of IFF
** 8SVX 8-bit sampled audio data, plays the data from both files using just
** one channel.  This demonstrates how virtual audio channels can be
** implemented.
**
** The program supports two different methods for virtual voices.  Method 1
** (the default method) interleaves bytes from each file so that the data words
** fed into the Amiga’s audio hardware contain one byte each from the given
** files.  The samples are then played back at twice their normal speed.  Since
** each sample only gets half of the playback bandwidth, the speed sounds
** correct.  To the listener, it sounds as if both samples are playing
** simultaneously even though only one channel is used.
**
** Normally the maximum playback rate with the Amiga’s audio hardware is about
** 28K bytes/sec.  Since interleaving requires doubling the nominal sampling
** rate, it will only work with audio data created at a sampling rate of 14K
** bytes/sec or less.
**
** Method 2, takes one byte from each file, sums them and divides by two.
** The resulting byte value is sent to the Amiga’s audio hardware.  No speed
** increase is required for this technique, however some noise  is introduced
** by the averaging of the byte values.  To use method 2, inlcude the SUM
** keyword as the last argument typed on the command line.  Examples:
**
**    interplay talk.8svx music.8svx SUM  (Uses method 2, averaging)
**    interplay talk.8svx music.8svx      (Uses method 1, interleaving)
**    interplay talk.8svx                 (Normal single file 8SVX playback)
**
** For an example of conventional IFF 8SVX audio see the "Amiga ROM Kernel
** Reference Manual: Devices", 3rd edition (ISBN 0-201-56775-X), page 28 and
** page 515.
*/

#include <exec/types.h>
#include <exec/devices.h>
#include <exec/memory.h>
#include <devices/audio.h>
#include <dos/dos.h>

#include <iff/iff.h>
#include <iff/8svx.h>

#include <clib/exec_protos.h>
#include <clib/dos_protos.h>
#include <clib/alib_protos.h>

#include <stdio.h>
#include <string.h>
#include <dos.h>      /* This is the dos.h file from SAS/C not Commodore */

#ifdef SASC
int CXBRK(VOID)    { return(0); };
int chkabort(VOID) { return(0); };
#endif

                                                                                    #define BUF_SIZE 1024

                                                                                    /* Prototypes for functions defined in this program */
                                                                                    struct IOAudio *SiezeChannel( VOID );
                                                                                    VOID            ReleaseChannel( struct IOAudio * );
                                                                                    char           *Parse8svx(char *, struct InterPlay * );
                                                                                    VOID            EndParse( struct InterPlay * );
                                                                                    VOID            FillAudio(struct InterPlay *, struct IOAudio * );

                                                                                    struct InterPlay                      /* This is the main structure used for */
                                                                                        {                                 /*  storage of playback state info.    */
                                                                                        ULONG             sample_done;    /* 0=Keep playing, 1=all done playing. */
                                                                                        UBYTE            *sample_byte;    /* Pointer for going through the data. */
                                                                                        UBYTE            *sample_loc;     /* Start of 8SVX BODY data in memory.  */
                                                                                        ULONG             sample_size;    /*  and total size of file for freeing.*/
                                                                                        struct InterPlay *next_iplay;     /* Link to second data set. NULL means */
                                                                                                                          /*  no second file name was given.     */
                                                                                        LONG              offsetBody;     /* Offset into the file of BODY Chunk. */
                                                                                        UWORD             sample_speed;   /* Value for audio period register.    */
                                                                                        BOOL              USE_SUMMING;    /* TRUE means use averaging,           */
                                                                                        };                                /*  FALSE means use interleaving.      */

                                                                                    /* Version string for AmigaDOS VERSION command. */
                                                                                    UBYTE versiontag[] = "$VER: Interplay 1.0 (2.2.93)";

                                                                                    /*-----------------------------------------
                                                                                    **
                                                                                    **          main()
                                                                                    **
                                                                                    **-----------------------------------------
                                                                                    */

                                                                                    VOID main(int argc, char **argv)
                                                                                    {
                                                                                    struct InterPlay  mainplay,otherplay;   /* Two instances of the InterPlay    */
                                                                                                                            /*  structure, one for each file.    */
                                                                                    struct IOAudio *pIOA_1=NULL,
                                                                                                   *pIOA_2=NULL,            /* Two IOAudio pointers, plus one    */
                                                                                                   *pIOA  =NULL;            /*  for switching back and forth     */
                                                                                    struct MsgPort *mport1=NULL,            /*  during double-buffering.         */
                                                                                                   *mport2=NULL,            /* Two MsgPort pointers, plus one    */
                                                                                                   *mport =NULL;            /*  for switching back and forth.    */

                                                                                    struct Message *msg;                    /* For the GetMsg() call.            */

                                                                                    LONG aswitch = 0L;                      /* Double-buffering logical switch.  */

                                                                                    static BYTE chip playbuffer1[BUF_SIZE]; /* Two buffers, one for each IOAudio */
                                                                                    static BYTE chip playbuffer2[BUF_SIZE]; /*  request.  Play out of one while  */
                                                                                                                            /*  the other is being set up.       */
                                                                                    char *errormsg;     /* For error returns */
                                                                                    ULONG wakemask=0L;  /* For Wait() call   */

                                                                                    /* Give an AmigaDOS style help message */
                                                                                    if( (argc == 2) && !strcmp(argv[1],"?\0") )
                                                                                        printf("8SVX-FILES/M,SUM/S\n");

Amiga Mail

Page VI - 8 Sound and Music Creating Virtual Voices with Amiga Audio

else if(argc>=2) /* OK got at least one argument. */
    {

    /* Get an audio channel at the highest priority */
    if( pIOA_1=SiezeChannel() )
      {

      mport1 = pIOA_1->ioa_Request.io_Message.mn_ReplyPort;
      pIOA_1->ioa_Data = playbuffer1;

      /* Get a 2nd MsgPort and 2nd IOAudio structure for double-buffering */
      pIOA_2 = AllocMem(sizeof(struct IOAudio),MEMF_PUBLIC | MEMF_CLEAR );
      mport2 = CreatePort(0,0);

      if( pIOA_2 && mport2 )
          {
          /* The 2 IOAudio requests should be initialized the same */
          /* except for the buffer and the reply port they use.    */
          *pIOA_2 = *pIOA_1;
          pIOA_2->ioa_Request.io_Message.mn_ReplyPort = mport2;
          pIOA_2->ioa_Data = playbuffer2;

          /* Default is to use interleaving, not averaging */
          mainplay.USE_SUMMING = FALSE;

          /* Parse the 8SVX file and fill in the InterPlay structure */
          errormsg = Parse8svx( argv[1] , &mainplay );

          /* If a second file name was given by the user then this is */
          /* an interleave request, so parse the 2nd 8SVX file.       */
          if( argc>=3 && !errormsg )
              {
              errormsg = Parse8svx( argv[2] , &otherplay );
              mainplay.next_iplay = &otherplay;

              /* If the SUM keyword was given in the command line, set the */
              /* SUMMING flag so that averaging, not interleaving, is used.*/
              if( (argc == 4) &&
                  ( !strcmp(argv[3],"SUM\0") || !strcmp(argv[3],"sum\0") )  )
                  mainplay.USE_SUMMING = TRUE;
              }
          else
              otherplay.sample_done = 1;

          if(!errormsg) /* File names given parsed OK? */
              {
              /* Fill up the buffer for the first request. */
              FillAudio( &mainplay, pIOA_1);

              /* Is there enough data to double-buffer ? */
              if(!mainplay.sample_done || !otherplay.sample_done)
                  {
                  /* OK, enough data to double-buffer; fill up 2nd request */
                  FillAudio( &mainplay, pIOA_2 );
                  BeginIO((struct IORequest *) pIOA_1 );
                  BeginIO((struct IORequest *) pIOA_2 );

                  /* Initial state of double-buffering variables */
                  aswitch=0; pIOA=pIOA_2; mport=mport1;

                                                                                                      /*---------------------*/
                                                                                                      /*  M A I N   L O O P  */
                                                                                                      /*---------------------*/

                                                                                                      while(!mainplay.sample_done || !otherplay.sample_done)
                                                                                                          {
                                                                                                          wakemask=Wait( (1 << mport->mp_SigBit) |
                                                                                                                                   SIGBREAKF_CTRL_C  );

                                                                                                          if( wakemask & SIGBREAKF_CTRL_C )
                                                                                                              {
                                                                                                              otherplay.sample_done = 1;
                                                                                                              mainplay.sample_done = 1;
                                                                                                              }

                                                                                                          while((msg=GetMsg(mport))==NULL){}

                                                                                                          /* Toggle double-buffering variables */
                                                                                                          if  (aswitch) {aswitch=0;pIOA=pIOA_2;mport=mport1;}
                                                                                                          else          {aswitch=1;pIOA=pIOA_1;mport=mport2;}

                                                                                                          FillAudio( &mainplay, pIOA );
                                                                                                          BeginIO((struct IORequest *) pIOA );
                                                                                                          }

                                                                                                      wakemask=Wait( 1 << mport->mp_SigBit );
                                                                                                      while((msg=GetMsg(mport))==NULL){}

                                                                                                      if  (aswitch) {aswitch=0;pIOA=pIOA_2;mport=mport1;}
                                                                                                      else          {aswitch=1;pIOA=pIOA_1;mport=mport2;}

                                                                                                      wakemask=Wait( 1 << mport->mp_SigBit );
                                                                                                      while((msg=GetMsg(mport))==NULL){}
                                                                                                      }
                                                                                                  else
                                                                                                      {
                                                                                                      /* Only enough data to fill up one buffer */
                                                                                                      BeginIO((struct IORequest *) pIOA_1 );
                                                                                                      wakemask=Wait( 1 << mport1->mp_SigBit );
                                                                                                      while((msg=GetMsg(mport1))==NULL){}
                                                                                                      }
                                                                                                  }
                                                                                              else
                                                                                                  /* One or the other of the files had a problem in Parse8svx() */
                                                                                                  printf(errormsg);

                                                                                              /* Free the memory used for the 8SVX files in Parse8svx() */
                                                                                              if(mainplay.next_iplay)
                                                                                                  EndParse( &otherplay );
                                                                                              EndParse( &mainplay );

                                                                                              }
                                                                                          else printf("Couldn’t get memory for a second IOAudio and MsgPort\n");

                                                                                          /* Free the ports and memory used by the 2 IOAudio requests */
                                                                                          if(mport2) DeletePort(mport2);
                                                                                          if(pIOA_2) FreeMem( pIOA_2, sizeof(struct IOAudio) );

                                                                                          ReleaseChannel(pIOA_1);
                                                                                          }
                                                                                        else printf("Couldn’t get a channel on the audio device\n");
                                                                                        }
                                                                                    else printf("Enter one or two 8SVX filenames.\n");
                                                                                    }

Sound and Music

Amiga Mail

Page VI - 9 Creating Virtual Voices with Amiga Audio

/*----------------------------------------------------------------------
** struct IOAudio *res = SiezeChannel( VOID )
**
**   Allocates any channel at the highest priority.  Once allocated,
**   the hardware registers of the given channel can be hit directly
**   without interfering with normal audio.device operation.
**
**   Retruns NULL on failure
**   or returns the address of the IOAudio used to get the channel.
**   If the call to this function succeeds, ReleaseChannel() should
**   be called later to free the channel and memory used for the IOAudio.
**-----------------------------------------------------------------------
*/

struct IOAudio *
SiezeChannel( VOID )
{
struct IOAudio *myAIOreq=NULL;
struct MsgPort *myAIOreply=NULL;
UBYTE chans[] = {1,2,4,8};      /* Try to get one channel, any channel */
BYTE dev = -1;

myAIOreq=(struct IOAudio *)AllocMem(sizeof(struct IOAudio),MEMF_PUBLIC );
if(myAIOreq)
    {
    myAIOreply=CreatePort(0,0);
    if(myAIOreply)
        {
        myAIOreq->ioa_Request.io_Message.mn_ReplyPort   = myAIOreply;
        myAIOreq->ioa_Request.io_Message.mn_Node.ln_Pri = 127;
        myAIOreq->ioa_Request.io_Command                = ADCMD_ALLOCATE;
        myAIOreq->ioa_AllocKey                          = 0;
        myAIOreq->ioa_Data                              = chans;
        myAIOreq->ioa_Length                            = sizeof(chans);

        dev=OpenDevice("audio.device",0L,(struct IORequest *)myAIOreq,0L);

       if(! dev)
            return( myAIOreq ); /* Successful exit */

        DeletePort( myAIOreply );
        }
    FreeMem( myAIOreq, sizeof(struct IOAudio) );
    }
return( NULL );
}

/*---------------------------------------------------------------
** VOID ReleaseChannel(struct IOAudio *rel );
**
**   Frees the channel and any asociated memory allocated earlier
**   with SiezeChannel().
**---------------------------------------------------------------
*/

VOID
ReleaseChannel(struct IOAudio *rel)
{
if(rel)
    {
    CloseDevice( (struct IORequest *) rel );

                                                                                        if(rel->ioa_Request.io_Message.mn_ReplyPort)
                                                                                            {
                                                                                            DeletePort(rel->ioa_Request.io_Message.mn_ReplyPort);
                                                                                            }
                                                                                        FreeMem( rel, sizeof(struct IOAudio) );
                                                                                        }
                                                                                    }

                                                                                    /*--------------------------------------------------------------------
                                                                                    **
                                                                                    ** char *Parse8svx( char *filename, struct InterPlay *play_state)
                                                                                    **
                                                                                    **   Pass this function the name of an 8svx file.  It opens the file and
                                                                                    **   finds the VHDR and BODY Chunks.  Playback information is stored
                                                                                    **   in the InterPlay structure.
                                                                                    **
                                                                                    **   A NULL return indicates the parse was completely successful.
                                                                                    **   A non-NULL return means the file cannot be played back for
                                                                                    **   some reason.  In that case the return value is a pointer to
                                                                                    **   an error message explaining what went wrong.
                                                                                    **
                                                                                    **   After calling Parse8svx(), End Parse() should be called
                                                                                    **   to free any memory used.
                                                                                    **
                                                                                    **----------------------------------------------------------------------
                                                                                    */

                                                                                    char *
                                                                                    Parse8svx(char *fname, struct InterPlay *play)
                                                                                    {
                                                                                    BYTE iobuffer[12];
                                                                                    LONG rdcount=0L;
                                                                                    Chunk *pChunk=NULL;
                                                                                    GroupHeader *pGH=NULL;

                                                                                    Voice8Header *pV8Head = NULL;
                                                                                    char         *error   = NULL;
                                                                                    BPTR         filehandle=NULL;
                                                                                    BOOL         NO_BODY  = TRUE;
                                                                                    BOOL         NO_VHDR  = TRUE;

                                                                                    /* Under normal operation, this function leaves the file positioned */
                                                                                    /* at the BODY Chunk.  However, for some degenerate 8SVX files, one */
                                                                                    /* additional seek is needed at the end.  In that case this field   */
                                                                                    /* (play->offsetBody) will be changed to the seek offset.           */
                                                                                    play->offsetBody = 0;
                                                                                    play->sample_loc = NULL;   /* Set to non-NULL if memory is allocated  */
                                                                                    play->next_iplay = NULL;   /* Default is no successors, no interleave */
                                                                                    play->sample_done= 0L;     /* Will be set to 1 when playback is done  */

                                                                                    filehandle= NULL;          /* Set to non-NULL if the file opens       */

                                                                                    NO_BODY=TRUE;
                                                                                    NO_VHDR=TRUE;

                                                                                    /* This section just makes sure that the first 12 bytes of the */
                                                                                    /* file conform to the IFF FORM specification, sub-type 8SVX.  */
                                                                                    filehandle = Open( fname, MODE_OLDFILE );
                                                                                    if(filehandle)
                                                                                        {
                                                                                        /* Next, read the first 12 bytes to check the type */

Amiga Mail

Page VI - 10 Sound and Music Creating Virtual Voices with Amiga Audio

    rdcount =Read( filehandle, iobuffer, 12L );
    if(rdcount==12L)
        {
        /* Make sure it is an IFF FORM type */
        pGH = (GroupHeader *)iobuffer;
        if(pGH->ckID == FORM)
            {
            /* Make sure it is an 8SVX sub-type */
            if(pGH->grpSubID != ID_8SVX)
                    error="Not an 8SVX file\n";
            }
        else
            error="Not an IFF FORM\n";
        }
    else
        error="Read error or file too short1\n";
    }
else
    error="Couldn’t open that file. Try another.\n";

/* Read through all Chunks until BODY and VHDR */
/* Chunks are found or until an error occurs.  */
while( !error &&   (NO_BODY  ||  NO_VHDR) )
    {
    /* Read the first 8 bytes of the Chunk to get the type and size */
    rdcount =Read( filehandle, iobuffer, 8L );
    if(rdcount==8L)
        {
        pChunk=(Chunk *)iobuffer;
        switch(pChunk->ckID)
            {

            case ID_VHDR:
                /* AllocMem() ckSize rounded up and read */
                /* the VHDR, filling in the InterPlay */
                if(pChunk->ckSize & 1L)
                    pChunk->ckSize++;

                pV8Head = AllocMem(pChunk->ckSize, MEMF_PUBLIC);
                if(pV8Head)
                    {
                    rdcount=Read(filehandle,pV8Head,pChunk->ckSize);
                    if(rdcount==pChunk->ckSize )
                        {
                        if(pV8Head->sCompression==sCmpNone)
                            {
                            /* Set the playback speed */
                            play->sample_speed = (UWORD)
                                        (3579545L / pV8Head->samplesPerSec);

                            /* Set up start, end of sample data */
                            play->sample_size = pV8Head->oneShotHiSamples
                                                   + pV8Head->repeatHiSamples;
                            }
                        else error="Can’t read compressed file\n";
                        }
                    else error="Read problem in header\n";

                    FreeMem(pV8Head, pChunk->ckSize );
                    }
                else error="Couldn’t get header memory\n";
                NO_VHDR = FALSE;
                break;

                                                                                                case ID_BODY:
                                                                                                    /* Technically, a VHDR could come after a BODY.*/
                                                                                                    /* This is a pretty unlikely occurence though. */
                                                                                                    if(NO_VHDR)
                                                                                                        {
                                                                                                        if(pChunk->ckSize & 1L)
                                                                                                            pChunk->ckSize++;

                                                                                                        rdcount = Seek(filehandle, pChunk->ckSize, OFFSET_CURRENT);
                                                                                                        if(rdcount==-1)
                                                                                                            error="Problem during BODY-skipping seek\n";
                                                                                                        else
                                                                                                            play->offsetBody=rdcount;
                                                                                                        }
                                                                                                    NO_BODY = FALSE;
                                                                                                    break;

                                                                                                default:
                                                                                                    /* Ignore other Chunks, skipping over them */
                                                                                                    if(pChunk->ckSize & 1L)
                                                                                                        pChunk->ckSize++;

                                                                                                    rdcount = Seek(filehandle, pChunk->ckSize, OFFSET_CURRENT);
                                                                                                    if(rdcount==-1)
                                                                                                        error="Problem during chunk-skipping seek\n";
                                                                                                    break;
                                                                                                }
                                                                                            }
                                                                                        else error = "Read error or file too short2\n";
                                                                                        }

                                                                                    if(!error)
                                                                                        {
                                                                                        /* In case the VHDR came after the BODY, seek back to the BODY */
                                                                                        if(play->offsetBody)
                                                                                            {
                                                                                            rdcount = Seek(filehandle, play->offsetBody, OFFSET_BEGINNING);
                                                                                            if(rdcount==-1)
                                                                                                error="Couldn’t seek to BODY\n";
                                                                                            }

                                                                                        /* OK now get the BODY data into a memory block */
                                                                                        play->sample_loc = AllocMem( play->sample_size, MEMF_PUBLIC );
                                                                                        if(play->sample_loc)
                                                                                            {
                                                                                            rdcount = Read(filehandle, play->sample_loc, play->sample_size);
                                                                                            if(rdcount!=play->sample_size)
                                                                                                error = "Error during BODY read\n";
                                                                                            else
                                                                                                play->sample_byte=play->sample_loc;
                                                                                            }
                                                                                        else
                                                                                            error="Couldn’t get memory for BODY Chunk\n";
                                                                                        }

                                                                                    if(filehandle)
                                                                                        Close(filehandle);

                                                                                    return(error);
                                                                                    }

Sound and Music

Amiga Mail

Page VI - 11 Creating Virtual Voices with Amiga Audio

/*---------------------------------------------------------------
**
** VOID EndParse( struct InterPlay * );
**
**   This function simply frees any memory used by an earlier
**   call to Parse8svx().
**
**---------------------------------------------------------------
*/
VOID
EndParse( struct InterPlay *play )
{
if(play->sample_loc)
    FreeMem(play->sample_loc, play->sample_size );
}

/*-----------------------------------------------------------------------------
**
** VOID FillAudio(struct InterPlay *, struct IOAudio * );
**
**   This function gets 512 bytes each from 2 BODY buffers and interleaves
**   the bytes in the audio playback buffer.
**-----------------------------------------------------------------------------
-
*/
VOID
FillAudio(struct InterPlay *inplay, struct IOAudio *ioa )
{
struct InterPlay *play1,*play2;
ULONG remainder1,remainder2,x;
UWORD speedfac;
WORD value;

if(ioa->ioa_Request.io_Command != CMD_WRITE) /* For 1st time callers only */
    {
    /* When two files are played at once, their speeds must match.  Use  */
    /* whichever speed is fastest. Interleaved requests also require the */
    /* speed to be doubled (period is halved).  However, the period      */
    /* cannot be lower than 124 or audio DMA bandwidth will be exceeded. */
    speedfac = inplay->sample_speed;

    if(inplay->next_iplay)
        {
        if(inplay->next_iplay->sample_speed < inplay->sample_speed)
            speedfac = inplay->next_iplay->sample_speed;

        if ( !(inplay->USE_SUMMING) )
            speedfac /= 2;
        }

    if(speedfac < 124)
        speedfac = 124;

    ioa->ioa_Request.io_Command = CMD_WRITE;
    ioa->ioa_Request.io_Flags   = ADIOF_PERVOL;
    ioa->ioa_Volume             = 63;
    ioa->ioa_Period             = speedfac;
    ioa->ioa_Length             = BUF_SIZE;
    ioa->ioa_Cycles             = 1;
    }

if(inplay->next_iplay)

                                                                                        {
                                                                                        play1=inplay;
                                                                                        play2=inplay->next_iplay;

                                                                                        remainder1 = play1->sample_size - (play1->sample_byte - play1->sample_loc);
                                                                                        remainder2 = play2->sample_size - (play2->sample_byte - play2->sample_loc);

                                                                                        if(play1->USE_SUMMING)
                                                                                            {
                                                                                            /*
                                                                                            ** AVERAGING LOGIC for playing TWO samples on ONE channel
                                                                                            */
                                                                                            for(x=0; x<BUF_SIZE ;x++)
                                                                                                {
                                                                                                value = 0;

                                                                                                if( x<remainder1 )
                                                                                                    {
                                                                                                    value += *( (BYTE *)(play1->sample_byte) );
                                                                                                    play1->sample_byte++;
                                                                                                    }
                                                                                                else if( x==remainder1 )
                                                                                                    play1->sample_done=1;

                                                                                                if( x<remainder2 )
                                                                                                    {
                                                                                                    value += *( (BYTE *)(play2->sample_byte) );
                                                                                                    play2->sample_byte++;
                                                                                                    }
                                                                                                else if( x==remainder2 )
                                                                                                    play2->sample_done=1;

                                                                                                *(ioa->ioa_Data + x) = (UBYTE) (value/2);
                                                                                                }
                                                                                            }
                                                                                        else
                                                                                            {
                                                                                            /*
                                                                                            ** INTERLEAVE LOGIC for playing TWO samples on ONE channel
                                                                                            */

                                                                                           /* If there are more bytes in the 1st sample data file, place them in */
                                                                                           /* the EVEN positions in the playback buffer of this IOAudio request. */
                                                                                            for(x=0; (x<BUF_SIZE) && (x<2*remainder1); x+=2 )
                                                                                                {
                                                                                                *(ioa->ioa_Data + x) = *(play1->sample_byte);
                                                                                                play1->sample_byte++;
                                                                                                }
                                                                                            /* If there are no more bytes then mark the 1st sample as done */
                                                                                            if(x<BUF_SIZE)
                                                                                                play1->sample_done=1L;

                                                                                            while(x<BUF_SIZE)      /* Pad the playback buffer with zeroes. */
                                                                                                {
                                                                                                *(ioa->ioa_Data + x) = 0;
                                                                                                x+=2;
                                                                                                }

                                                                                           /* If there are more bytes in the 2nd sample data file, place them in */
                                                                                           /* the ODD positions in the playback buffer of this IOAudio request.  */
                                                                                            for(x=1; (x<BUF_SIZE) && (x<2*remainder2);x+=2)
                                                                                                {
                                                                                                *(ioa->ioa_Data + x) = *(play2->sample_byte);
                                                                                                play2->sample_byte++;
                                                                                                }

Amiga Mail

Page VI - 12 Sound and Music Creating Virtual Voices with Amiga Audio

        /* If there are no more bytes then mark the 2nd sample as done */
        if(x<BUF_SIZE)
            play2->sample_done=1L;

        while(x<BUF_SIZE)      /* Pad the playback buffer with zeroes. */
            {
            *(ioa->ioa_Data + x) = 0;
            x+=2;
            }
        }
    }
else
    {
    /*
    ** REGULAR LOGIC for playing a single sample on a single channel.
    */
    remainder1= inplay->sample_size - (inplay->sample_byte-inplay->sample_loc);
    if(remainder1 > BUF_SIZE)
        {
        CopyMem(inplay->sample_byte,ioa->ioa_Data,BUF_SIZE);
        inplay->sample_byte+=BUF_SIZE;
        }
    else
        {
        CopyMem(inplay->sample_byte,ioa->ioa_Data,remainder1);
        ioa->ioa_Length=remainder1;
        inplay->sample_done=1L;
        }
    }
}

∞∞