Sending;¬DPT 2021 ISA SCSI Adapter
¬

¬SCSI Devices

ISA Bus

Supported Hardware: 
	PM2021 ISA SCSI Adapter 
   PM2041W ISA Wide SCSI Adapter
   
This driver supports the DPT PM 2021 and PM2041W ISA SCSI Host Adapters.

Before you install a DPT ISA SCSI Host Adapter, you must first run the Configure application to configure the driver.  Be sure to write down the settings for DMA channel, IRQ, and Port Address obtained from the Configure Application before you install the host adapter itself. 

Installing a DPT PM2021or PM2041W ISA SCSI Adapter

1.	Refer to the "Smart Cache User's Manual" that comes with the adapter.  This manual contains information that you should read before installing the adapter.  
2.  For the PM2021 SCSI Adapter, configure the jumpers for I/O Address, DRQ (DMA Channel), and IRQ to match the values selected in the configure App, as described above. For the PM2041W Host Adapter, the I/O address, DMA Channel, and IRQ are set via the DPT's on-board Configuration program, which is run at boot time. 
3.   Be aware of the necessity of proper SCSI termination.  Refer to 
       the User's Manual and configure the host adapter accordingly. 
4.	Install the DPT ISA SCSI Adapter in an ISA slot.
5.	Restart your computer.  It will use the new adapter as you configured it. 

¬
	
See also

·	"Add a Device" in Configure's on-line help.

·	See NeXTanswer  1824 for general information on installing 
	and configuring device drivers. 

·	See NeXTanswer 1830 for an overview of this DPT device 
	driver.