SoundBlaster8 Audio Driver

This driver is for 8-bit Sound Blaster compatible series cards. It will work with Sound Blaster Classic, Sound Blaster 2.0 and Sound Blaster Pro cards. 

The range of sampling rates is limited by hardware capabilities of these cards. However some clone cards may not be able support higher rates.

             Playback            Recording
Classic       4-23 KHz             4-13 KHz
2.0          4-44.1 KHz           4-15 KHz
Pro          4-44.1 KHz           4-44.1 KHz
  
Also note that the Pro card can playback in stereo but only upto 22KHz. 
 
Playback of compressed sound files is not supported.

You should make sure that DMA/IRQ/Port Address selected using Configure is same as the one defined by the jumpers on the sound card. Refer to the hardware documentation for available jumpers and how to set them.