SoftPC 4.0 with Windows
FOR NEXTSTEP FOR INTEL PROCESSORS

Installation Instructions:

1. Log in as "root" on the machine on which you want to install SoftPC.

2. Insert the SoftPC 4.0 CD-ROM.

3. Double-click the SoftPC.pkg icon to launch the Installer and install the SoftPC package.

4. Refer to page 7 of the SoftPC 4.0 Addendum for information on NEXTSTEP operating system patches which may need to be installed on your system.

To Run SoftPC 4.0:

1. Log in using your normal account.

2. Double-click the SoftPC icon to launch SoftPC.

3. Click OK in the Unlicensed SoftPC panel.

4. Enter your SoftPC license number and authorization code, or click the Demo button for a 30-day product trial.

5. Create a new hard disk file. You will need at least 3MB for a DOS disk and 13MB for a Windows disk. You should add the hard disk space you require for installing PC applications to these figures. Please refer to the SoftPC User Guide for further information.

6. SoftPC will now start, and you can use it just as you would a real PC.