XAmode   (c)1993 KNOPS EDV-Anlagen Gerd Knops, Germany

This program enables you to read PHOTO-CDs with a  TOSHIBA CD-ROM 
(This program is not  required for the Type 3501)

Usage:

	XAmode -t#

        where # is a substitution for the device address (0..6) of  the CD-ROM drive

This program must be executed with superuser right. Therefore you must be logged in as ªrootº when launching it.

XAmode can be executed immediately before reading a Photo-CD or automatically when starting up your computer.

Follow these steps:

1. Log in as ªrootº.
2. If the folder /usr/local/bin doesnÂt exist yet, create it.
3. Copy the program  ªXAmodeº to /usr/local/bin
4. Add the following line at the end of the file ª/etc/rc.localº (This line is only necessary if you want XAmode to be loaded automatically each time you start your computer.)

	/usr/local/bin/XAmode -t#
	
        where # is a substitution for the device address (0..6) of  the CD-ROM drive

Note: It might happen that the SCSI devices are reinitialized during a work session (e.g. if there are errors when reading from the harddisk). If this happens, you must execute XAmode again.